{"text_format":"1","workbook":"xlsx","n_sheets":20,"sheets":["ToC - LEGEND","Roadmap","LTB","SG - Switch","SG - SFP Tranceiver","SG - Device Server","SG - Wireless AP & C","SG - Antenna  Accessory ","Competition Switch","Competition DeviceServer","DS - Managed Switch","DS - Lite Managed Switch ","DS - Proview Switch","DS - Unmanaged Switch","DS - PoE  Switch","DS - Train Switch","DS - Device Server","DS - Media Converter","DS - Wireless Connectivity","DS - NMS"],"not_rendered":{"charts":0,"images":8,"macros":1,"external_links":1,"defined_names":25,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ToC - LEGEND","index":0,"n_rows":23,"n_cols":3,"rows_kept":23,"cut":false,"hidden":false,"merged":[[22,0,22,1]]}
["ITEM (CLICK the Hyperlinks below)","TAB NAME","PURPOSE"]
["Table of Contents - Legend","ToC - Legend","Provides you an overview and hyperlinks for direct navigation to each TAB by click"]
["Roadmap New Product","Roadmap","Shows you planed release dates for new products"]
["Last Time Buy","LTB","Provides you with end of live info per part number when relevant"]
["Selection Guide - Switches","SG - Switch","Guides you to find the matching Switch product"]
["Selection Guide - SFP Transceiver","SG - SFP Transceiver","Guides you to find the matching SFP Transceiver product"]
["Selection Guide - Device Server","SG - Device Server","Guides you to find the matching Device Server product"]
["Selection Guide - Wireless & Celular Connectivity","SG - Wireless AP & C","Guides you to find the matching WiFi AP/Client & Cellular Gatewat/Router product"]
["Selection Guide - Wireless Antennas and Accessories","SG - Antenna  Accessory ","Guides you to find the matching Wireless Antenna & Accessoires product"]
["Competition Matrix Switches","Competition Switch","Privides you a table showing Advantech Switch compared to competitive model"]
["Competition Matrix Device Servers","Competition Device Server","Privides you a table showing Advantech Device Server compared to competitive model"]
["Datasheets & Features - Managed Switches","DS - Managed Switch","Shows Feature List of Managed Switches"]
["Datasheets & Features - Proview Switches","DS - ProView Switch","Shows Feature List of ProView Switches"]
["Datasheets & Features - Unmanaged Switches","DS - Unmanaged Switch","Shows Feature List of Unmanaged Switches"]
["Datasheets & Features - Power over Ethernet  Switches","DS - PoE Switch","Shows Feature List of PoE Switches"]
["Datasheets & Features - Train Switches","DS - Train Switch","Shows Feature List of Train Switches"]
["Datasheets & Features - Device Servers","DS - Device Server","Shows Feature List of Device Servers"]
["Datasheets & Features - Media Converters","DS - Media Converter","Shows Feature List of Media Converters"]
["Datasheets & Features - WiFi & Celular Connectivity","DS - Wiereless Connectivity","Shows Feature List of WiFi AP/Client & Celular Gateway/Router"]
["Datasheets & Features - Webaccess NMS","DS - NMS","Shows Feature List of Webaccess/NMS - Network Management Software"]
[]
[]
["CLICK the \"BACK to ToC\" BUTTON in each TAB to RETURN to \"ToC - LEGEND\" TAB"]

{"sheet":"Roadmap","index":1,"n_rows":58,"n_cols":6,"rows_kept":58,"cut":false,"hidden":false,"merged":[[40,0,41,0],[42,0,43,0],[44,0,45,0],[1,0,4,0],[5,0,8,0],[11,0,17,0],[5,3,6,3],[7,3,8,3],[46,0,51,0],[52,0,57,0],[18,0,23,0],[24,0,29,0],[30,0,35,0],[36,0,37,0],[38,0,39,0],[5,1,6,1],[5,2,6,2],[7,1,8,1],[7,2,8,2],[9,0,10,0]]}
["Product Type","Model","Function","MP Schedule","MP Q'ty","PM"]
["EKI-2706","EKI-2706E-1G1FP","4FE +1GE+1 Fiber  -10 ~ 60℃ ","2015-05-25",30,"Nisha Lin"]
[null,"EKI-2706E-1G1FPI","4FE +1GE+1 Fiber wide temp","2015-05-25",30,"Nisha Lin"]
[null,"EKI-2706G-1G1FP","4GE +1GE+1 Fiber  -10 ~ 60℃ ","2015-05-25",30,"Nisha Lin"]
[null,"EKI-2706G-1G1FPI","4GE +1GE+1 Fiber wide temp","2015-05-25",30,"Nisha Lin"]
["EKI-2725","EKI-2725-CE","5GE -10 ~ 60℃","2016-06-11","TBD","Nisha Lin"]
[null,null,null,null,"TBD","Nisha Lin"]
[null,"EKI-2725I-CE","5GE wide temp","2016-06-11","TBD","Nisha Lin"]
[null,null,null,null,"TBD","Nisha Lin"]
["EKI-9228","EKI-9228G-8CMI-AE","16GE + 8Combo + 4SFP 48VDC input","2016-07-08","TBC","Nisha Lin"]
[null,"EKI-9228G-8COI-AE","16GE + 8Combo + 4SFP\nHigh voltage ACDC input","2016-07-15",30,"Nisha Lin"]
["EKI-5528","EKI-5528-EI-AE","8 x FE RJ-45 EIP","2016-05-06",20,"Nisha Lin"]
[null,"EKI-5528I-EI-AE","8 x FE RJ-45 EIP Wide Temp.","2016-05-06",30,"Nisha Lin"]
[null,"EKI-5528-MB-AE","8 x FE RJ-45 Modbus","2016-05-06",20,"Nisha Lin"]
[null,"EKI-5528I-MB-AE","8 x FE RJ-45 Modbus Wide Temp.","2016-05-06",30,"Nisha Lin"]
[null,"EKI-5528-PN-AE","8 x FE RJ-45 PIO","2016/6/31",20,"Nisha Lin"]
[null,"EKI-5528I-PN-AE","8 x FE RJ-45 PIO Wide Temp.","2016/6/31",20,"Nisha Lin"]
[null,"EKI-5528-PNMA","8 x FE RJ-45 PIO MRP Master","2016/6/31",20,"Nisha Lin"]
["EKI-5629","EKI-5629C-EI-AE","8 x FE RJ-45+2GE Combo EIP","2016-05-06",20,"Nisha Lin"]
[null,"EKI-5629CI-EI-AE","8 x FE RJ-45+2GE Combo EIP Wide Temp.","2016-05-06",30,"Nisha Lin"]
[null,"EKI-5629C-MB-AE","8 x FE RJ-45+2GE Combo Modbus","2015-05-06",20,"Nisha Lin"]
[null,"EKI-5629CI-MB-AE","8 x FE RJ-45+2GE Combo Modbus Wide Temp.","2015-05-06",30,"Nisha Lin"]
[null,"EKI-5629C-PN-AE","8 x FE RJ-45+2GE Combo PIO","2016/6/31",20,"Nisha Lin"]
[null,"EKI-5629CI-PN-AE","8 x FE RJ-45+2GE Combo PIO Wide Temp.","2016/6/31",20,"Nisha Lin"]
["EKI-5526","EKI-5526-EI-AE","16 x FE RJ-45 EIP","2016-05-06",0,"Nisha Lin"]
[null,"EKI-5526I-EI-AE","16 x FE RJ-45 EIP Wide Temp.","2016/3/B\n2016/4/15\n2016/5/6",20,"Nisha Lin"]
[null,"EKI-5526-MB-AE","16 x FE RJ-45 Modbus","2015-05-06",0,"Nisha Lin"]
[null,"EKI-5526I-MB-AE","16 x FE RJ-45 Modbus Wide Temp.","2015-05-06",20,"Nisha Lin"]
[null,"EKI-5526-PN-AE","16 x FE RJ-45 PIO","2016/6/31",20,"Nisha Lin"]
[null,"EKI-5526I-PN-AE","16 x FE RJ-45 PIO Wide Temp.","2016/6/31",20,"Nisha Lin"]
["EKI-5626","EKI-5626C-EI-AE","16 x FE RJ-45+2GE Combo EIP","2016-05-06",0,"Nisha Lin"]
[null,"EKI-5626CI-EI-AE","16 x FE RJ-45+2GE Combo EIP Wide Temp.","2016-05-06",20,"Nisha Lin"]
[null,"EKI-5626C-MB-AE","16 x FE RJ-45+2GE Combo MGT","2016-05-06",0,"Nisha Lin"]
[null,"EKI-5626CI-MB-AE","16 x FE RJ-45+2GE Combo MGT Wide Temp","2016-05-06",20,"Nisha Lin"]
[null,"EKI-5626C-PN-AE","16 x FE RJ-45+2GE Combo PIO","2016/6/31",20,"Nisha Lin"]
[null,"EKI-5626CI-PN-AE","16 x FE RJ-45+2GE Combo PIO Wide Temp.","2016/6/31",20,"Nisha Lin"]
["EKI-1528DR(FCI)","EKI-1528I-DR-AE","8-port RS-232/422/485 Din Rail Serial Device Server with wide Temp. ","\n2016/4/15",30,"Nisha Lin"]
[null,"EKI-1528CI-DR-AE","8-port RS-232/422/485 Din Rail Serial Device Server with wide temp & iso ","2016-04-15",30,"Nisha Lin"]
["USB-4604B(M)-BE","USB-4604B-BE","4-Port RS-232 to USB Converter ","2016-03-22","TBD","Nisha Lin"]
[null,"USB-4604BM-BE","4-Port RS-232/422/485 to USB Converter ","2016-03-22","TBD","Nisha Lin"]
["Proneer Switch\n16G+4SPF","EKI-7720G-4F-AE","Proneer 16G + 4SFP -10 ~ 60℃ ","2016-06-04","30","Steve.Wang"]
[null,"EKI-7720G-4FI-AE","Proneer 16G + 4SFP wide temp","2016-06-04","30","Steve.Wang"]
["Proneer Switch\n16FE+4SFP","EKI-7720E-4F-AE","Proneer 16FE+4SFP -10 ~ 60℃ ","2016-06-04","30","Steve.Wang"]
[null,"EKI-7720E-4FI-AE","Proneer 16FE+4SFP wide temp","2016-06-04","30","Steve.Wang"]
["Train switch","EKI-5609E-1GPI-AE","8FE+1G POE wide temp","2016/3/M",null,"Steve.Wang"]
[null,"EKI-7612E-4GPI-AE","8FE+4G POE wide temp","2016/3/M",null,"Steve.Wang"]
["Train switch","EKI-9516-P0IDH10E","16GE POE wide temp\nHigh voltage input","2016/8/B",null,"Steve.Wang"]
[null,"EKI-9516-P0IDL10E","16GE POE wide temp\nLow voltage input","2016/8/B",null,"Steve.Wang"]
[null,"EKI-9516-C0IDW10E","16GE w/o POE wide temp\nWide voltage input","2016/8/B",null,"Steve.Wang"]
[null,"EKI-9512-P0IDH10E","12GE POE wide temp\nHigh voltage input","2016/8/B",null,"Steve.Wang"]
[null,"EKI-9512-P0IDL10E","12GE POE wide temp\nLow voltage input","2016/8/B",null,"Steve.Wang"]
[null,"EKI-9512-C0IDW10E","12GE w/o POE wide temp\nWide voltage input","2016/8/B",null,"Steve.Wang"]
["Train switch","EKI-9516-PFIDH10E","16FE POE wide temp\nHigh voltage input","2016/8/B",null,"Steve.Wang"]
[null,"EKI-9516-PFIDL10E","16FE POE wide temp\nLow voltage input","2016/8/B",null,"Steve.Wang"]
[null,"EKI-9516-CFIDW10E","16FE w/o POE wide temp\nWide voltage input","2016/8/B",null,"Steve.Wang"]
[null,"EKI-9512-PFIDH10E","12FE POE wide temp\nHigh voltage input","2016/8/B",null,"Steve.Wang"]
[null,"EKI-9512-PFIDL10E","12FE POE wide temp\nLow voltage input","\n2016/8/B",null,"Steve.Wang"]
[null,"EKI-9512-CFIDW10E","12FE w/o POE wide temp\nWide voltage input","2016/8/B",null,"Steve.Wang"]

{"sheet":"LTB","index":2,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["Model","Issue Date","Last-Buy Date","Last-Buy Qty","Last Shipment","Successor","Note"]
[]
["EKI-2548I-AE","2015-07-31","2015-10-30",null,"2016-01-29","EKI-7710E-2CI-AE"]
["EKI-1221D-AE","2015-08-25","2015-09-22",null,"2015-12-15","EKI-1221-BE+ EKI-2525"]
["EKI-1222D-AE","2015-08-25","2015-09-22",null,"2015-12-15","EKI-1222-BE+ EKI-2525"]
["EKI-6311GN-AE","2015-12-03","2016-02-26",null,"2016-12-31","EKI-6332GN-AE"]
["EKI-6311GN-EU-AE","2015-12-03","2016-02-26",null,"2016-08-26","EKI-6332GN-EU-AE"]
["EKI-6331AN-AE","2015-12-03","2016-02-26",null,"2016-08-26","EKI-6331AN-BE"]
["EKI-6331AN-EU-AE","2015-12-03","2016-02-26",null,"2016-08-26","EKI-6331AN-EU-BE"]
["EKI-6310GN-AE","2015/8/28","2015/8/28",null,"2015/8/28","N/A"]
["EKI-6340-1A-AE ","2016-02-18","2016-03-18",null,"2016-08-26"]
["EKI-6340-2A-AE ","2016-02-18","2016-03-18",null,"2016-08-26"]
["EKI-6340-3A-AE ","2016-02-18","2016-03-18",null,"2016-08-26"]
["EKI-6340-1U-AE ","2016-02-18","2016-03-18",null,"2016-08-26"]
["EKI-6340-2U-AE ","2016-02-18","2016-03-18",null,"2016-08-26"]
["EKI-6340-3U-AE ","2016-02-18","2016-03-18",null,"2016-08-26"]
["EKI-6351-A-AE ","2016-02-18","2016-03-18",null,"2016-08-26"]

{"sheet":"SG - Switch","index":3,"n_rows":104,"n_cols":15,"rows_kept":104,"cut":false,"hidden":false,"merged":[[1,5,1,6],[1,7,1,11],[1,12,1,13]]}
[]
[null,null,null,null,null,"RJ-45",null,"Fiber",null,null,null,null,"PoE"]
["Function","Type ","Product","Description","Port Numbers","10/100 Mbps ","Gigabit ","10/100 Mbps ","Gigabit ","GE Combo ports","Type","Connector","PoE RJ-45 (10/100 Mbps)","PoE RJ-45(Gigabit)","Wide temp/Normal temp"]
["Managed","DIN-Rail","EKI-7710E-2C","8FE+2G Port Gigabit Managed Redundant Industrial Switch",10,"8",null,null,null,"2","SFP",null,null,null,"N"]
["Managed","DIN-Rail","EKI-7710E-2CI","8FE+2G Port Gigabit Managed Redundant Industrial Switch w/wide temp",10,"8",null,null,null,"2","SFP",null,null,null,"W"]
["Managed","DIN-Rail","EKI-7710G-2C","8G+2G Port Gigabit Managed Redundant Industrial Switch",10,null,"8",null,null,"2","SFP",null,null,null,"N"]
["Managed","DIN-Rail","EKI-7710G-2CI","8G+2G Port Gigabit Managed Redundant Industrial Switch w/wide temp",10,null,"8",null,null,"2","SFP",null,null,null,"W"]
["Managed","DIN-Rail","EKI-2548I","8Tx Managed Ethernet Switch with Wide Temperature","8","8",null,null,null,null,null,null,null,null,"W"]
["Managed","DIN-Rail","EKI-2748CI","6Gx+2 Combo Managed Ethernet Switch with Wide Temperature","8",null,"6",null,null,"2","SFP",null,null,null,"W"]
["Managed","DIN-Rail","EKI-2748FI","4Gx+4SFP Managed Ethernet Switch with Wide Temperature","8",null,"4",null,"4",null,"SFP",null,null,null,"W"]
["Managed","Rack","EKI-7428G-4CI","24G+4G Combo port L2 Managed Switch","28",null,"24",null,null,"4","SFP",null,null,null,"W"]
["Managed","DIN-Rail","EKI-7554MI","4+2 SC Type Fiber Optic Managed Industrial Ethernet Switch with Wide Temperature","6","4",null,"2",null,null,"Multi-mode","SC",null,null,"W"]
["Managed","DIN-Rail","EKI-7554SI","4+2 SC Type Fiber Optic Managed Industrial Ethernet Switch with Wide Temperature","6","4",null,"2",null,null,"Single-mode","SC",null,null,"W"]
["Managed","DIN-Rail","EKI-7559MI","8+2 SC Type Fiber Optic Managed Industrial Ethernet Switch with Wide Temperature","10","8",null,"2",null,null,"Multi-mode","SC",null,null,"W"]
["Managed","DIN-Rail","EKI-7559SI","8+2 SC Type Fiber Optic Managed Industrial Ethernet Switch with Wide Temperature","10","8",null,"2",null,null,"Single-mode","SC",null,null,"W"]
["Managed","DIN-Rail","EKI-7654C","4+2G Combo Port Gigabit Managed Redundant Industrial Ethernet Switch","6","4",null,null,null,"2","SFP",null,null,null,"N"]
["Managed","DIN-Rail","EKI-7656C","16+2G Combo Port Gigabit Managed Redundant Industrial Ethernet Switch","18","16",null,null,null,"2","SFP",null,null,null,"N"]
["Managed","DIN-Rail","EKI-7656CI","16+2G Combo Port Gigabit Managed Redundant Industrial Ethernet Switch w/ Wide Temp","18","16",null,null,null,"2","SFP",null,null,null,"W"]
["Managed","DIN-Rail","EKI-7657C","7+3G Combo Port Gigabit Managed Redundant Industrial Ethernet Switch with 2 x DI/O","10","7",null,null,null,"3","SFP",null,null,null,"N"]
["Managed","DIN-Rail","EKI-7657CI","7+3G Combo Port Gigabit Managed Redundant Industrial Ethernet Switch with 2 x DI/O","10","7",null,null,null,"3","SFP",null,null,null,"W"]
["Managed","DIN-Rail","EKI-7659C","8+2G Combo Port Gigabit Managed Redundant Industrial Ethernet Switch",10,"8",null,null,null,"2","SFP",null,null,null,"N"]
["Managed","DIN-Rail","EKI-7659CI","8+2G Combo Port Gigabit Managed Redundant Industrial Ethernet Switch w/ Wide Temp",10,"8",null,null,null,"2","SFP",null,null,null,"W"]
["Managed","DIN-Rail","EKI-7758F","4G+4 SFP Gigabit Managed Redundant Industrial Ethernet Switch","8",null,"4",null,"4",null,"SFP",null,null,null,"N"]
["Managed","DIN-Rail","EKI-9312","8G+4G Port Gigabit Managed Redundant Industrial Switch","12",null,"8",null,"4",null,"SFP",null,null,null,"W"]
["Managed","DIN-Rail","EKI-9316","12G+4G Port Gigabit Managed Redundant Industrial Switch","16",null,"12",null,"4",null,"SFP",null,null,null,"W"]
["Managed","DIN-Rail","EKI-7710E-2CP","8FE+2G Port Gigabit Managed Redundant Industrial PoE+ Switch",10,null,null,null,null,"2","SFP",null,"8",null,"N"]
["Managed","DIN-Rail","EKI-7710E-2CPI","8FE+2G Port Gigabit Managed Redundant Industrial PoE+ Switch w/wide temp",10,null,null,null,null,"2","SFP",null,"8",null,"W"]
["Managed","DIN-Rail","EKI-7710G-2CP","8G+2G Port Gigabit Managed Redundant Industrial PoE+ Switch",10,null,null,null,null,"2","SFP",null,null,"8","N"]
["Managed","DIN-Rail","EKI-7710G-2CPI","8G+2G Port Gigabit Managed Redundant Industrial PoE+ Switch w/wide temp",10,null,null,null,null,"2","SFP",null,null,"8","W"]
["Managed","Rack","EKI-7428G-4CPI","24G+4G Combo port L2 Managed PoE Switch","28",null,null,null,null,"4","SFP",null,null,"24","W"]
["Managed","DIN-Rail","EKI-7659CPI","8+2G Port Gigabit Managed Redundant Industrial PoE Switch with Wide Temperature",10,null,null,null,null,"2","SFP",null,"8",null,"W"]
["Managed","DIN-Rail","EKI-9312P","8G+4G Port Gigabit Managed Redundant Industrial PoE+ Switch","12",null,null,null,"4",null,"SFP",null,null,"8","W"]
["Managed","DIN-Rail","EKI-9316P","12G+4G Port Gigabit Managed Redundant Industrial PoE+ Switch","16",null,null,null,"4",null,"SFP",null,null,"12","W"]
["Unmanaged / Proview","DIN-Rail","EKI-5525","5-port Fast Ethernet ProView Switch","5","5",null,null,null,null,null,null,null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5525I","5-port Fast Ethernet ProView Switch with Wide Temperature","5","5",null,null,null,null,null,null,null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5525S","4-port +1x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch","5","4",null,"1",null,null,"Single-mode","SC",null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5525SI","4-port +1x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch","5","4",null,"1",null,null,"Single-mode","SC",null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5525S-ST","4-port +1x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch","5","4",null,"1",null,null,"Single-mode","ST",null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5525SI-ST","4-port +1x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch","5","4",null,"1",null,null,"Single-mode","ST",null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5525M","4-port +1x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch","5","4",null,"1",null,null,"Multi-mode","SC",null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5525MI","4-port +1x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch","5","4",null,"1",null,null,"Multi-mode","SC",null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5525M-ST","4-port +1x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch","5","4",null,"1",null,null,"Multi-mode","ST",null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5525MI-ST","4-port +1x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch","5","4",null,"1",null,null,"Multi-mode","ST",null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5528","8-port Fast Ethernet ProView Switch","8","8",null,null,null,null,null,null,null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5528I","8-port Fast Ethernet ProView Switch with Wide Temperature","8","8",null,null,null,null,null,null,null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5629C","8FE + 2GE Combo Ethernet ProView Switch","10","8",null,null,null,"2","SFP",null,null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5629CI","8FE + 2GE Combo Ethernet ProView Switch","10","8",null,null,null,"2","SFP",null,null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5725","5-port Gigabit Ethernet ProView Switch","5",null,"5",null,null,null,null,null,null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5725I","5-port Gigabit Ethernet ProView Switch with Wide Temperature","5",null,"5",null,null,null,null,null,null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5728","8-port Gigabit Ethernet ProView Switch","8",null,"8",null,null,null,null,null,null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5728I","8-port Gigabit Ethernet ProView Switch with Wide Temperature","8",null,"8",null,null,null,null,null,null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5726","16-port Gigabit Ethernet ProView Switch","16",null,"16",null,null,null,null,null,null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5726I","16-port Gigabit Ethernet ProView Switch w/wide temp","16",null,"16",null,null,null,null,null,null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5626C","16FE + 2GE Combo Ethernet ProView Switch","18","16",null,null,null,"2","SFP"]
["Unmanaged / Proview","DIN-Rail","EKI-5626CI","16FE + 2GE Combo Ethernet ProView Switch w/wide temp","18","16",null,null,null,"2","SFP"]
["Unmanaged / Proview","DIN-Rail","EKI-5524SS","4-port + 2x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch","6","4",null,"2",null,null,"Single-mode","SC",null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5524SSI","4-port + 2x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch w/wide temp","6","4",null,"2",null,null,"Single-mode","SC",null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5524SS-ST","4-port + 2x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch","6","4",null,"2",null,null,"Single-mode","ST",null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5524SSI-ST","4-port + 2x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch w/wide temp","6","4",null,"2",null,null,"Single-mode","ST",null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5726F","16-port+2 SFP Gigabit Ethernet ProView Switch","18",null,"16",null,"2",null,"SFP",null,null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5726FI","16-port+2 SFP Gigabit Ethernet ProView Switch w/wide temp","18",null,"16",null,"2",null,"SFP",null,null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5729F","8-Port+2 SFP Gigabit Ethernet ProView Switch","10",null,"8",null,"8",null,"SFP",null,null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5729FI","8-Port+2 SFP Gigabit Ethernet ProView Switch w/wide temp","10",null,"8",null,"8",null,"SFP",null,null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5524MM","4-port + 2x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch","6","4",null,"2",null,null,"Multi-mode","SC",null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5524MMI","4-port + 2x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch w/wide temp","6","4",null,"2",null,null,"Multi-mode","SC",null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5524MM-ST","4-port + 2x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch","6","4",null,"2",null,null,"Multi-mode","ST",null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5524MMI-ST","4-port + 2x100FX port (Single/Multi-mode, SC/ST type), Fast Ethernet ProView Switch w/wide temp","6","4",null,"2",null,null,"Multi-mode","ST",null,null,"W"]
["Unmanaged / Proview","DIN-Rail","EKI-5526","16-port Fast Ethernet ProView Switch","16","16",null,null,null,null,null,null,null,null,"N"]
["Unmanaged / Proview","DIN-Rail","EKI-5526I","16-port Fast Ethernet ProView Switch w/wide temp","16","16",null,null,null,null,null,null,null,null,"W"]
["Unmanaged","DIN-Rail","EKI-2525","5-port Unmanaged Industrial Ethernet Switch","5","5",null,null,null,null,null,null,null,null,"N"]
["Unmanaged","DIN-Rail","EKI-2525I","5-port Unmanaged Industrial Ethernet Switch w/ Wide Temp","5","5",null,null,null,null,null,null,null,null,"W"]
["Unmanaged","DIN-Rail","EKI-2525M","4+1 100FX Port Multi-Mode Unmanaged Industrial Ethernet Switch","5","4",null,"1",null,null,null,null,null,null,"N"]
["Unmanaged","DIN-Rail","EKI-2526M","4+2 100FX Port Unmanaged Industrial Ethernet Switch","6","4",null,"2",null,null,"Multi-mode","SC",null,null,"N"]
["Unmanaged","DIN-Rail","EKI-2526S","4+2 100FX Port Single Mode Unmanaged Industrial Ethernet Switch","6","4",null,"2",null,null,"Single-mode","SC",null,null,"N"]
["Unmanaged","DIN-Rail","EKI-2528","8-port Unmanaged Industrial Ethernet Switch","8","8",null,null,null,null,null,null,null,null,"N"]
["Unmanaged","DIN-Rail","EKI-2528I","8-port Unmanaged Industrial Ethernet Switch w/ Wide Temp","8","8",null,null,null,null,null,null,null,null,"W"]
["Unmanaged","DIN-Rail","EKI-2725","5-port Gigabit Unmanaged Industrial Ethernet Switch","5",null,"5",null,null,null,null,null,null,null,"N"]
["Unmanaged","DIN-Rail","EKI-2728","8-port Gigabit Unmanaged Industrial Ethernet Switch","8",null,"8",null,null,null,null,null,null,null,"N"]
["Unmanaged","DIN-Rail","EKI-2728I","8-port Gigabit Unmanaged Industrial Ethernet Switch","8",null,"8",null,null,null,null,null,null,null,"W"]
["Unmanaged","DIN-Rail","EKI-2728MI","6Gx+2 Multi-Mode Unmanaged Ethernet Switch with Wide Temperature","8",null,"6",null,"2",null,"Multi-mode","SC",null,null,"W"]
["Unmanaged","DIN-Rail","EKI-3525","5-port 10/100Mbps Unmanaged Industrial Ethernet Switch","5","5",null,null,null,null,null,null,null,null,"N"]
["Unmanaged","DIN-Rail","EKI-3528","8-port 10/100Mbps Unmanaged Industrial Ethernet Switch","8","8",null,null,null,null,null,null,null,null,"N"]
["Unmanaged","DIN-Rail","EKI-3725","5-port Gigabit Unmanaged Industrial Ethernet Switch","5",null,"5",null,null,null,null,null,null,null,"N"]
["Unmanaged","DIN-Rail","EKI-3728","8-port Gigablte Unmanaged Industrial Ethernet Switch","8",null,"8",null,null,null,null,null,null,null,"N"]
["Unmanaged","Rack","EKI-4524I","24-port Ethernet Switch with Wide Temperature","24","24",null,null,null,null,null,null,null,null,"W"]
["Unmanaged","Rack","EKI-4524RI","24+2 SFP Port Unmanaged Industrial Ethernet Switch with Wide Temperature","26","24",null,"2",null,null,"SFP",null,null,null,"W"]
["Unmanaged","DIN-Rail","EKI-7526I","16-port Unmanaged Industrial Ethernet Switch with Wide Temperature","16","16",null,null,null,null,null,null,null,null,"W"]
["Unmanaged","DIN-Rail","EKI-7529MI/ST ","8+2 Multi-mode Fiber Optic Industrial Unmanaged Ethernet Switch with Wide Temperature","10","8",null,"2",null,null,"Multi-mode","ST",null,null,"W"]
["Unmanaged","DIN-Rail","EKI-7626C","16+2G Combo Port Gigabit Unmanaged Industrial Ethernet Switch","18","16",null,null,null,"2","SFP",null,null,null,"N"]
["Unmanaged","DIN-Rail","EKI-7626CI","16+2G Combo Port Gigabit Unmanaged Industrial Ethernet Switch","18","16",null,null,null,"2","SFP",null,null,null,"W"]
["Unmanaged","DIN-Rail","EKI-7629C","8+2G Combo Port Gigabit Unmanaged Industrial Ethernet Switch","10","8",null,null,null,"2","SFP",null,null,null,"N"]
["Unmanaged","DIN-Rail","EKI-7629CI","8+2G Combo Port Gigabit Unmanaged Industrial Ethernet Switch w/ Wide Temp","10","8",null,null,null,"2","SFP",null,null,null,"W"]
["Unmanaged","DIN-Rail","EKI-7629CP","8+2G Combo Port Gigabit Unmanaged Industrial Ethernet PoE Switch","10",null,null,null,null,"2","SFP",null,"8",null,"N"]
["Unmanaged","DIN-Rail","EKI-7629CPI","8+2G Combo Port Gigabit Unmanaged Industrial Ethernet PoE Switch","10",null,null,null,null,"2","SFP",null,"8",null,"W"]
["Unmanaged","DIN-Rail","EKI-2525P","5-port Industrial PoE Switch","5","1",null,null,null,null,null,null,"4",null,"N"]
["Unmanaged","DIN-Rail","EKI-2525PA","5-port Industrial PoE Switch with 24/48 VDC Power Input","5","1",null,null,null,null,null,null,"4",null,"N"]
["Unmanaged","DIN-Rail","EKI-2526PI","6-port Industrial PoE Switch with Wide Temperature","6","2",null,null,null,null,null,null,"4",null,"W"]
["Unmanaged","DIN-Rail","EKI-2528PAI","8-port Industrial PoE Switch with 24/48 VDC Power Input and Wide Temperature","8",null,null,null,null,null,null,null,"8",null,"W"]
["Unmanaged","DIN-Rail","EKI-7712E-4F","8FE+4SFP Managed Redundant Industrial Switch","12","8",null,null,"4",null,"SFP",null,null,null,"N"]
["Unmanaged","DIN-Rail","EKI-7712E-4FI","8FE+4SFP Managed Redundant Industrial Switch w/wide temp","12","8",null,null,"4",null,"SFP",null,null,null,"W"]
["Unmanaged","DIN-Rail","EKI-7712G-4F","8G+4SFP Gigabit Managed Redundant Industrial Switch","12",null,"8",null,"4",null,"SFP",null,null,null,"N"]
["Unmanaged","DIN-Rail","EKI-7712G-4FI","8G+4SFP Gigabit Managed Redundant Industrial Switch w/wide temp","12",null,"8",null,"4",null,"SFP",null,null,null,"W"]
["Unmanaged","DIN-Rail","EKI-7712G-4FP","8G+4SFP Gigabit Managed Redundant Industrial PoE+ Switch","12",null,null,null,"4",null,"SFP",null,null,"8","N"]
["Unmanaged","DIN-Rail","EKI-7712G-4FPI","8G+4SFP Gigabit Managed Redundant Industrial PoE+ Switch w/wide temp","12",null,null,null,"4",null,"SFP",null,null,"8","W"]

{"sheet":"SG - SFP Tranceiver","index":4,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[[12,5,13,5],[6,3,7,3],[6,5,7,5],[2,3,3,3],[4,3,5,3],[2,4,3,4],[4,4,5,4],[6,4,7,4],[2,0,5,0],[6,0,19,0],[6,1,7,1],[8,1,9,1],[14,1,15,1],[18,1,19,1],[16,1,17,1],[10,1,11,1],[12,1,13,1],[18,3,19,3],[8,3,9,3],[10,3,11,3],[12,3,13,3],[12,4,13,4],[14,4,15,4],[16,4,17,4],[18,4,19,4],[16,3,17,3],[14,3,15,3],[8,4,9,4],[10,4,11,4],[18,5,19,5],[2,6,3,6],[4,6,5,6],[6,6,7,6],[8,6,9,6],[10,6,11,6],[12,6,13,6],[14,6,15,6],[16,6,17,6],[18,6,19,6],[14,5,15,5],[16,5,17,5],[2,5,3,5],[4,5,5,5],[8,5,9,5],[10,5,11,5],[16,7,17,7],[18,7,19,7],[2,7,3,7],[4,7,5,7],[8,7,9,7],[10,7,11,7],[12,7,13,7],[14,7,15,7],[6,7,7,7]]}
["Subject: SFP (mini-GBIC) Model List"]
["Category","Distance","Model Name","Wavelength","TX Power","RX Sens","Link Budget","Voltage","Operating Temp","Monitor"]
["100Base-FX","M.M. (2km)","SFP-FXM/LC-AE","1310 nm","-14dBm ~ -20dBm","\"-31dBm (Min)\"","11dB","3.3V","0 to 70℃","--"]
[null,"M.M. (2km)","SFP-FXM/LCI-AE",null,null,null,null,null,"(-40 to 85℃)"]
[null,"S.M. (30km)","SFP-FXS/LC-30E","1310 nm","(-8 dBm ~ -15dBm)","\"-34dBm (Min)\"","11dB","3.3V","0 to 70℃","-"]
[null,"S.M. (30km)","SFP-FXS/LCI-30E",null,null,null,null,null,"(-40 to 85℃)"]
["1000Base","SX (550m)","SFP-GSX/LC-AE","850 nm","(-4 dBm ~ -9.5dBm)","\"-18dBm (Min)\"","19dB","3.3V","0 to 70℃","--"]
[null,null,"SFP-GSX/LCI-AE",null,null,null,null,null,"(-20 to 85℃)"]
[null,"LX (10 km)","SFP-GLX/LC-10E","1310 nm","(-3 dBm ~ -9.5dBm)","\"-20dBm (Min)\"","19dB","3.3V","0 to 70℃","--"]
[null,null,"SFP-GLX/LCI-10E",null,null,null,null,null,"(-40 to 85℃)"]
[null,"LX (20 km)","SFP-GLX/LC-20E","1310 nm","(-2 dBm ~ -8dBm)","\"-23dBm (Min)\"","19dB","3.3V","0 to 70℃","YES"]
[null,null,"SFP-GLX/LCI-20E",null,null,null,null,null,"(-40 to 85℃)"]
[null,"LX (40 km)","SFP-GLX/LC-40E","1310 nm","(+1 dBm ~ -4dBm)","\"-24dBm (Min)\"","20dB","3.3V","0 to 70℃","--"]
[null,null,"SFP-GLX/LCI-40E",null,null,null,null,null,"(-40 to 85℃)"]
[null,"XD (50km)","SFP-GXD/LC-50E","1550 nm","(+1 dBm ~ -4dBm)","\"-24dBm (Min)\"","20dB","3.3V","0 to 70℃","--"]
[null,null,"SFP-GXD/LCI-50E",null,null,null,null,null,"(-40 to 85℃)"]
[null,"ZX (70km)","SFP-GZX/LC-70E","1550 nm","(+5 dBm ~ 0dBm)","\"-24dBm (Min)\"","20dB","3.3V","0 to 70℃"]
[null,null,"SFP-GZX/LCI-70E",null,null,null,null,null,"(-40 to 85℃)"]
[null,"EZX (110km)","SFP-GZX/LC-110E","1550 nm","(+5 dBm ~ 0dBm)","\"30dBm (Min)\"","20dB","3.3V","0 to 70℃","--"]
[null,null,"SFP-GZX/LCI-110E",null,null,null,null,null,"(-40 to 85℃)"]
["1000Base","RJ45 (100m)","SFP-GTX/RJ45-AE",null,null,null,null,"3.3V","0 to 70℃","-"]

{"sheet":"SG - Device Server","index":5,"n_rows":15,"n_cols":12,"rows_kept":15,"cut":false,"hidden":false,"merged":[[1,8,1,9],[1,10,1,11],[3,0,7,0],[3,1,6,1],[8,0,12,0],[8,1,11,1],[0,0,2,1],[0,2,0,11],[1,2,1,3],[1,4,1,5],[1,6,1,7]]}
[null,null,"Serial device server"]
[null,null,"1 Port",null,"2 Port",null,"4 Port",null,"8 Port",null,"16 Port"]
[null,null,null,"W-Temp.",null,"W-Temp.",null,"W-Temp.",null,"W-Temp.",null,"W-Temp."]
["Device Server","Standard","EKI-1521-AE",null,"EKI-1522-AE",null,"EKI-1524-AE",null,"EKI-1528",null,"EKI-1526"]
[null,null,"ADAM-4570",null,"ADAM-4571"]
[null,null,"ADAM-4570L",null,"ADAM-4571L",null,null,null,"EKI-1528T-VDC",null,"EKI-1526T-VDC"]
[null,null,"EKI-1521-BE","EKI-1521I-BE","EKI-1522-BE","EKI-1522I-BE","EKI-1524-BE","EKI-1524I-BE"]
[null,"Isolation",null,"EKI-1521CI-BE",null,"EKI-1522CI-BE",null,"EKI-1524CI-BE"]
["Modbus Gateway","Standard","ADAM-4572",null,"EKI-1222-AE",null,"EKI-1224-AE"]
[null,null,"EKI-1221-AE"]
[]
[null,null,"EKI-1221-BE","EKI-1221I-BE","EKI-1222-BE","EKI-1222I-BE","EKI-1224-BE","EKI-1224I-BE"]
[null,"Isolation",null,"EKI-1221CI-BE",null,"EKI-1222CI-BE",null,"EKI-1224CI-BE"]
[]
[null,"New release Product"]

{"sheet":"SG - Wireless AP & C","index":6,"n_rows":21,"n_cols":9,"rows_kept":21,"cut":false,"hidden":false,"merged":[[0,0,1,1],[0,3,0,4],[0,6,1,6],[2,0,9,0],[2,1,9,1],[2,6,3,6],[4,6,5,6],[10,0,14,0],[10,1,14,1],[15,0,18,0],[15,1,18,1],[20,1,20,2]]}
["WiFi",null,"Dual Band","Single Band",null,null,"Cellular","GPRS","3G"]
[null,null,"2.4G+5G","2.4G","5G",null,null,"850/900/1800/1900","850/900/1800/1900/2100"]
["Outdoor","AP",null,null,null,null,"Gateway","　 EKI-1321","　 EKI-1331"]
[null,null,null,null,null,null,null,"　EKI-1322"]
[null,null,null,null,null,null,"Router",null,"　EKI-1334"]
[]
[]
[]
[]
[]
["Indoor","AP/Client",null,"EKI-6332GN","　EKI-6331AN"]
[]
[]
[]
[]
["Indoor","Client",null,"EKI-1361"]
[null,null,null,"EKI-1362"]
[null,null,null,"EKI-6232GN"]
[]
[]
[null,"New release Product"]

{"sheet":"SG - Antenna  Accessory ","index":7,"n_rows":35,"n_cols":4,"rows_kept":35,"cut":false,"hidden":false,"merged":[]}
[]
[]
["Advantech P/N","ANT-2216M-G2E","ANT-2216M-G5E"]
["Frequency Range","2.4-2.5G","5.1-5.9G"]
["Antenna Type","Patch","Patch"]
["Antenna Gain","16 dBi","16 dBi"]
["Impedance","50 Ohm","50 Ohm"]
["Polarization","Linear, vertical/horizontal","Linear, vertical"]
["HPBW/Vertical","25/25","19/21"]
["V.S.W.R.","2.0:1 (Max.)","2.0:1 (Max.)"]
["Power Handling","6 W (cw)","6 W (cw)"]
["Connector","N-Jack","N-Jack"]
["Conntector Q'ty","1900-01-02","1900-01-02"]
["Operating temp.","-40 to +80","-40 to +80"]
["IP rating","IP67","IP55"]
["Weight","1.1 kg","0.8 kg"]
[]
[]
[]
["Advantech P/N","ANT-5130","ANT-5230"]
["Description","3M N-Plug to SMA-Plug cable","3M N-Plug to N-Plug cable"]
["Cable Type","ULA-168","ULA400"]
["VSWR","1.5 : 1 Max.@ DC~3.0 GHz\n2.0 : 1 Max.@ 3.0~6.0 GHz","1.5 : 1 Max.@ DC~6.0 GHz"]
["Insertion loss","3.5 dB Max.@ DC~3.0 GHz\n4 dB Max.@ 3.0~6.0 GHz","1.1 dB Max.@ DC~3 GHz\n1.6 dB Max.@ 3~6.0 GHz"]
["Connector Type","N-plug to RP SMA-plug","N-plug to N-plug"]
["Cable Length","3M","3M"]
[]
[]
[]
["Advantech P/N","ANT-5501","ANT-5502","ANT-5601"]
["Description","1KV Surge Arrestor N-Jack to N-Jack","1KV Surge Arrestor N-Plug to N-Jack","Bulkhead adapter N-Jack to N-Jack"]
["Surge Protection","1KV","1KV","N/A"]
["VSWR","1.25:1 Max @DC~4GHz\n1.45:1 Max @4~6GHz","1.3:1 Max @DC~4GHz\n1.5:1 Max @4~6GHz","1.2:1 Max @DC~3GHz\n1.4:1 Max @3~6GHz"]
["Insertion loss","0.8 dB","0.8 dB","N/A"]
["Connector Type","N Jack to N Jack","N plug to N Jack","N-jack to N-jack"]

{"sheet":"Competition Switch","index":8,"n_rows":77,"n_cols":12,"rows_kept":77,"cut":false,"hidden":false,"merged":[[61,6,62,6],[63,1,64,1],[63,2,64,2],[65,1,66,1],[67,0,76,0],[67,1,72,1],[67,2,69,2],[70,2,71,2],[73,1,76,1],[74,2,75,2],[56,0,66,0],[56,1,56,2],[57,1,62,1],[57,2,59,2],[60,2,62,2],[34,0,55,0],[34,1,40,1],[34,2,35,2],[36,2,40,2],[41,1,47,1],[42,2,45,2],[46,2,47,2],[48,1,53,1],[48,2,50,2],[54,1,55,2],[0,0,0,2],[1,0,33,0],[1,1,22,1],[1,2,10,2],[11,2,16,2],[17,2,22,2],[23,1,28,1],[23,2,28,2],[29,1,31,1],[30,2,31,2],[32,1,33,2]]}
["Category",null,null,"Advantech","Hirschmann","Siemens","MOXA","Phoenix Contact","N-Tron","Korenix","GarrettCom","Ruggedcom"]
["Unmanaged Industrial Ethernet Switch","10/100","5 Ports","ADAM-6520","RS2-5TX\n","SCALANCE X005\nSCALANCE XB005","EDS-205","FL Switch 5TX","105TX-SL","JetNet 2005"]
[null,null,null,"ADAM-6520I","N/A","SCALANCE X005TS","EDS-205A-T","FL Switch SFNT 5TX","105TX-SL","JetNet 2005-w"]
[null,null,null,"ADAM-6520L","RS2-5TX","SCALANCE X005\nSCALANCE XB005","EDS-205","FL Switch 5TX","105TX-SL","JetNet 2005"]
[null,null,null,"ADAM-6521","RS2-4TX/1FX EEC (wide-temp)\nSPIDER 4TX/1FX","N/A","EDS-205A-M-SC","FL Switch 4TX/FX","105FX-SC","JetNet 2005f-m"]
[null,null,null,"ADAM-6521S","RS2-4TX/1FX-SM EEC (wide-temp)\nSPIDER 4TX/1FX-SM EEC (wide-temp)","N/A","EDS-205A-S-SC","N/A","105FXE-SC","JetNet 2005f-s"]
[null,null,null,"ADAM-6521/ST","SPIDER 4TX/1FX-SM EEC (wide-temp)","N/A","EDS-205A-M-ST","FL Switch SFN 4TX/FX ST","105FX-ST","N/A"]
[null,null,null,"EKI-2525\nEKI-5525","RS2-5TX\nSPIDER 5TX","SCALANCE X005\nSCALANCE XB005","EDS-205\nEDS-205A\nEDS-305","FL Switch SFNB 5TX\nFL Switch SFN 5TX\nFL Switch 5TX\nFL Switch 5TX-ZF","105TX\n105TX-SL","JetNet 2005"]
[null,null,null,"EKI-2525I\nEKI-5525I","SPIDER 5TX EEC","SCALANCE X005TS","EDS-205A-T\nEDS-305-T","FL Switch SFNT 5TX","105TX\n105TX-SL","JetNet 2005-w"]
[null,null,null,"EKI-2525M\nEKI-5525M","RS2-4TX/1FX EEC (wide-temp)\nSPIDER 4TX/1FX EEC (wide-temp)","N/A","EDS-205A-M-SC\nEDS-305-M-SC","FL Switch SFNB 4TX/FX\nFL Switch SFN 4TX/FX\nFL Switch 4TX/FX","105FX-SC","JetNet 2005f-m"]
[null,null,null,"EKI-5525M-ST","SPIDER 4TX/1FX-ST EEC (wide-temp)","N/A","EDS-205A-M-ST\nEDS-305-M-ST","FL Switch SFNB 4TX/FX ST\nFL Switch SFN 4TX/FX ST","105FX-ST","N/A"]
[null,null,"6-9 Ports","EKI-2526M","RS2-3TX/2FX EEC (wide-temp, one-port less)","SCALANCE X104-2","N/A","N/A","106FX2-SC","N/A"]
[null,null,null,"EKI-2526M-ST","N/A","N/A","N/A","N/A","106FX2-ST","N/A"]
[null,null,null,"EKI-2526S","RS2-3TX/2FX-SM EEC (wide-temp, one-port less)","N/A","N/A","N/A","106FXE2-SC","N/A"]
[null,null,null,"EKI-2526S-ST","N/A","N/A","N/A","N/A","106FXE2-ST","N/A"]
[null,null,null,"EKI-2528\nEKI-5528","RS2-TX\nRS20-0800T1T1SDAUHH\nSPIDER 8TX\nSPIDER II 8TX","SCALANCE X108\nSCALANCE XB008","EDS-208\nEDS-208A\nEDS-308","FL Switch SFNB 8TX\nFL Switch SFN 8TX\nFL Switch 8TX","108TX","JetNet 3008"]
[null,null,null,"EKI-2528I\nEKI-5528I","SPIDER 8TX EEC\nSPIDER II 8TX EEC","N/A","EDS-208A-T\nEDS-308-T","FL Switch SFNT 8TX","108TX","JetNet 3008"]
[null,null,"10 Ports or Above","EKI-7526I","RS20-1600T1T1SDAUHH (normal temp.)","SCALANCE X116","EDS-316T","FL Switch SFNT 16TX","116TX","N/A"]
[null,null,null,"EKI-7526MI","RS20-1600M2M2SDAUHH (normal temp.)","N/A","N/A","FL Switch SFNT 14TX/2FX (two less ports)","N/A","N/A"]
[null,null,null,"EKI-7529MI","SPIDER II 8TX/2FX EEC","N/A","N/A","N/A","110FX2-SC","N/A"]
[null,null,null,"EKI-7529MI/ST","SPIDER II 8TX/2FX-ST EEC","N/A","N/A","N/A","110FX2-ST","N/A"]
[null,null,null,"EKI-4524I","No rackmountable model","No rackmountable model","IKS-6324","N/A","N/A","N/A"]
[null,null,null,"EKI-4524RI","No rackmountable model","No rackmountable model","N/A","N/A","N/A","N/A"]
[null,"10/100 + GE Uplink","10 Ports or Above","EKI-7629C","RS30-0802T1T1SDAUHH\nRS30-0802O6O6SDAUHH","N/A","N/A","N/A","N/A","JetNet 3010G (7 + 3G)"]
[null,null,null,"EKI-7629CI","N/A","N/A","N/A","N/A","N/A","JetNet 3010G (7 + 3G)"]
[null,null,null,"EKI-7629CP","N/A","N/A","N/A","N/A","N/A","N/A"]
[null,null,null,"EKI-7629CPI","N/A","N/A","N/A","N/A","N/A","N/A"]
[null,null,null,"EKI-7626C","RS30-1602T1T1SDAUHH\nRS30-1602O6O6SDAUHH","N/A","N/A","N/A","N/A","JetNet 3018G"]
[null,null,null,"EKI-7626CI","N/A","N/A","N/A","N/A","N/A","JetNet 3018G"]
[null,"Gigabit","5 Ports","EKI-2725\nEKI-5725","SPIDER II Giga 5T EEC (wide-temp)","SCALANCE XB005G","EDS-G205","N/A","1005TX","JetNet 3005G"]
[null,null,"8 Ports","EKI-2728\nEKI-5728","N/A","SCALANCE XB008G","EDS-G308","FL Switch SFN 8GT","N/A","JetNet 3008G"]
[null,null,null,"EKI-2728MI","N/A","N/A","EDS-G308-2SFP-T","FL Switch SFN 6GT/2SX","N/A","N/A"]
[null,"M12 EN50155",null,"EKI-6528TI","OCTOPUS 8M Train (IP67)","N/A","TN-5308-LV-T","N/A","108M12","JetNet 3006-M12 (Two ports less)\nJetNet 2006-M12 (Two ports less)"]
[null,null,null,"EKI-6528TPI","OCTOPUS 8M-6PoE (IP67, no EN50155)","N/A","TN-5308-4PoE-48-T","N/A","N/A","N/A"]
["Managed Redundant Industrial Ethernet Switch","10/100","4 + 2 Ports","EKI-7554MI","RS20-0400M2T1SDA (two ports less)","SCALANCE X204-2TS (BFOC Connecotor)","N/A","FL Switch LM 4TX/2FX","N/A","JetNet 4006f-mw"]
[null,null,null,"EKI-7554SI","N/A","N/A","N/A","FL Switch LM 4TX/2FX SM","N/A","JetNet 4006f-sw"]
[null,null,"8 Ports","EKI-2548I","RS20-0800T1T1SDA (normal temp.)","SIPLUS NET SCALANCE X208","EDS-408A-T","FL Switch LM 8TX","508TX-A\n708TX","JetNet 4508-w V2"]
[null,null,null,"EKI-2548MI","RS20-0800M2M2SDA (normal temp.)","N/A","EDS-408A-MM-SC-T","N/A","508FX2-A-SC\n708FX2-SC","JetNet 4508f-mw V2"]
[null,null,null,"EKI-2548SI","RS20-0800S2S2SDA (normal temp.)","N/A","EDS-408A-SS-SC-T","N/A","508FXE2-A-SC\n708FXE2-SC","JetNet 4508f-sw V2"]
[null,null,null,"EKI-7559MI","RS20-0900MMM2SDA (one-port less, normal temp)","SCALANCE X212-2 (two-port more, BFOC connector, normal temp)","N/A","N/A","710FX2-SC","JetNet 4508f-mw V2"]
[null,null,null,"EKI-7559SI","N/A","N/A","N/A","N/A","710FXE2-SC","JetNet 4508f-sw V2"]
[null,"10/100 + GE Uplink","4 + 2 Ports","EKI-7654C","N/A","SCALANCE X304-2FE","N/A","N/A","N/A","N/A"]
[null,null,"8 -10 Ports","EKI-7657C","N/A","SCALANCE X307-3\nSCALANCE X308-2\nSCALANCE X308-2LD\nSCALANCE X308-2LH\nSCALANCE X308-2LH+\nSCALANCE X310","EDS-510A","N/A","N/A","JetNet 5010G"]
[null,null,null,"EKI-7659C","RS30-0802T1T1SDA\nRS30-0802O6O6SDA","N/A","N/A","N/A","7010TX","N/A"]
[null,null,null,"EKI-7710E","RS30-0802T1T1SDA\nRS30-0802O6O6SDA","\nSCALANCE X308-2\nSCALANCE X308-2LD\nSCALANCE X308-2LH\nSCALANCE X308-2LH+\nSCALANCE X310FE","EDS-405A/408A\nEDS-505A/508A","N/A","7010TX","N/A"]
[null,null,null,"EKI-7659CI","N/A","N/A","N/A","N/A","7010TX","N/A"]
[null,null,"Up to 24 Ports","EKI-7656C","RS30-1602T1T1SDA\nRS30-1602O6O6SDA","SCALANCE X216 (no Gig uplink)","EDS-518A","FL Switch MCS 16TX (two ports less)\nFL Switch 14TX/2FX (two ports less)","7018TX","N/A"]
[null,null,null,"EKI-7656CI","N/A","N/A","EDS-518A-T","N/A","7018TX","N/A"]
[null,"GE","8 Ports","EKI-2748CI","N/A","N/A","N/A","FL Switch SMCS 8GT (Normal temp.)\nFL Switch SMCS 6GT/2SFP (Normal temp.)","N/A","JetNet 4508f-w V2"]
[null,null,null,"EKI-2748FI","N/A","N/A","N/A","N/A","N/A","N/A"]
[null,null,null,"EKI-7758F","N/A","N/A","N/A","N/A","N/A","N/A"]
[null,null,"8-10Ports","EKI-7710G","N/A","SCALANCE X310"," EDS-G508E\n EDS-G509","N/A","N/A","N/A"]
[null,null,"12Ports","EKI-9312",null,null,"EDS-608/611","N/A"]
[null,null,"16Ports","EKI-9316",null,null,"EDS-616\nEDS-516A","N/A"]
[null,"M12 EN50155",null,"EKI-6558TI","OCTOPUS 8M","SCALANCE X208PRO","TN-5508-LV-LV-T","N/A","708M12","JetNet 4506-M12 (Two ports less)"]
[null,null,null,"EKI-6559TMI","N/A","N/A","TN-5510-2GTXBP-LV-LV-T","N/A","N/A","N/A"]
["Power over Ethernet","PoE Splitter",null,"EKI-2701PSI","N/A","N/A","SPL-24 (10/100 only)","N/A","100-POE-SPL-CC (10/100 only)","N/A"]
[null,"10/100","5 Ports","EKI-2525P","N/A","N/A","N/A","N/A","105TX-POE","JetNet 3705"]
[null,null,null,"EKI-2525PA","N/A","N/A","N/A","N/A","N/A","JetNet 3705-24V"]
[null,null,null,"EKI-2525SPI","N/A","N/A","N/A","N/A","105FXE-SC-15-POE","JetNet 3705f-s"]
[null,null,"6-8 Ports","EKI-2526PI","N/A","N/A","EDS-P206A-4PoE","N/A","N/A","JetNet 3806G "]
[null,null,null,"EKI-2528PAI","N/A","N/A","EDS-P308","N/A","N/A","N/A"]
[null,null,null,"EKI-5624PI","N/A","N/A",null,"N/A","N/A","N/A"]
[null,"10/100 + GE Uplink","10 Ports","EKI-5729PI","N/A","N/A","N/A","N/A","N/A","JetNet 6810-RJ (EN50155)"]
[null,null,null,"EKI-7659CPI","N/A","N/A","N/A","N/A","N/A","JetNet 6810-RJ (EN50155)"]
[null,"GE","12 Ports","EKI-9312P",null,null,"EDS-P510A-8PoE\nEDS-G512E-8PoE\nEDS-P510","N/A"]
[null,null,"16 Ports","EKI-9316P",null,null,null,"N/A"]
["Ethernet Media Converter","10/100","Multi-mode","ADAM-6541","SPIDER 1TX/1FX","N/A","N/A","N/A","N/A","N/A"]
[null,null,null,"EKI-5541M","SPIDER 1TX/1FX","SCALANCE_X101-1","IMC-21-M-SC\nIMC-21A-M-SC","FL MC 10/100BASE-T/FO G1300","102MC-SC","JetCon 2301-m\nJetCon 1301-m"]
[null,null,null,"EKI-5541MI","SPIDER 1TX/1FX EEC","N/A","IMC-21A-M-SC-T","N/A","102MC-SC","By Request"]
[null,null,"Single-mode","EKI-2541S","SPIDER 1TX/1FX-SM","SCALANCE X101-1LD","IMC-21-S-SC","FL MC 10/100BASE-T/FO G1300 SM","102MCE-SC","JetCon 2301-s\nJetCon 1301-s"]
[null,null,null,"EKI-2541SI","SPIDER 1TX/1FX-SM EEC","N/A","IMC-21A-S-SC-T","N/A","102MCE-SC","By Request"]
[null,null,"WDM","ADAM-6542","N/A","N/A","N/A","N/A","N/A","N/A"]
[null,"Gigabit","Multi-mode","EKI-2741SX","N/A","N/A","N/A","N/A","N/A","N/A"]
[null,null,"Single-mode","EKI-2741LX","N/A","N/A","N/A","N/A","N/A","N/A"]
[null,null,null,"EKI-2741LXI","N/A","N/A","N/A","N/A","N/A","N/A"]
[null,null,"SFP","EKI-2741F","N/A","N/A","IMC-101G","N/A","1002MC","JetCon 3401G"]

{"sheet":"Competition DeviceServer","index":9,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[[0,0,1,3],[2,0,19,0],[2,1,13,1],[2,2,11,2],[2,3,4,3],[5,3,8,3],[12,2,13,2],[14,1,17,2],[14,3,15,3],[18,1,19,3]]}
["Category",null,null,null,"Advantech","MOXA","Digi","Lantronix","Phoenix Contact"]
[null,null,null,null,"ADAM-4571L","NPort 5110 (DB9)\nNport 5110A (DB9)","PortServer TS 1","N/A"," FL COMSERVER RS232"]
["Serial Device Server","Serial Device Server","Wired","1-Port","ADAM-4571","NPort 5130\nNPort 5130A\nNPort 5150\nNport 5150A","PortServer TS 1 MEI (Modbus supported)","UDS1100-IAP"," FL COMSERVER BASIC 232/422/485"]
[null,null,null,null,"EKI-1511","NPort 5130\nNPort 5130A\nNPort 5150\nNport 5150A","PortServer TS 1 MEI (Modbus supported)","UDS1100-IAP"," FL COMSERVER BASIC 232/422/485"]
[null,null,null,null,"EKI-1521","NPort IA5150\nNPort IA5150A","PortServer TS 1 MEI (Modbus supported)","XSDRSN-02\nXSDRIN-02"," FL COMSERVER BASIC 232/422/485"]
[null,null,null,"2-Port","ADAM-4570L","NPort 5210 (RJ45)\nNport 5210A (RS232)","PortServer TS 2","N/A","N/A"]
[null,null,null,null,"ADAM-4570","NPort 5230\nNPort 5232\nNPort 5230A\nNPort 5250A","PortServer TS 2 MEI (Modbus supported)","N/A","N/A"]
[null,null,null,null,"EKI-1512","NPort 5230\nNPort 5232\nNPort 5230A\nNPort 5250A","PortServer TS 2 MEI (Modbus supported)","N/A","N/A"]
[null,null,null,null,"EKI-1522","NPort IA5250\nNPort IA5250A","PortServer TS 2 MEI (Modbus supported)","XPress-DR+ (XSDR22000-01)","N/A"]
[null,null,null,"4-Port","EKI-1524","NPort 5410\nNPort 5430\nNPort 5450\nNPort IA5450\nNPort IA5450A","PortServer TS 4 MEI (Modbus supported)","N/A","N/A"]
[null,null,null,"8-Port","EKI-1528       (Rack)\nEKI-1528-DR (Din Rail )","CN2650-8\nNPort 5610-8\nNPort 5630-8\nNPort 5650-8","PortServer TS 8 MEI\nConnectPort TS 8\nConnectPort LTS 8W","N/A","N/A"]
[null,null,null,"16-Port","EKI-1526","CN2650-16\nNPort 5610-16\nNPort 5630-16\nNPort 5650-16","PortServer TS 16 MEI\nConnectPort TS 16\nConnectPort LTS 16W","N/A","N/A"]
[null,null,"Wireless","1-Port","EKI-1351\nEKI-1361","Nport W2150 Plus","ConnectPort TS 1W (Modbus supported)","N/A","N/A"]
[null,null,null,"2-Port","EKI-1352\nEKI-1362","Nport W2250 Plus","ConnectPort TS 2W (Modbus supported)","XPress-DR+ Wireless (XSDR22W00-01)","N/A"]
[null,"Modbus Gateway",null,"1-Port","ADAM-4572","MGate MB3180 ","ConnectPort TS 1W","N/A"," FL COMSERVER UNI 232/422/485"]
[null,null,null,null,"EKI-1221\nEKI-1221D","MGate MB3180\nMGate MB3170","PortServer TS 1 MEI","N/A"," FL COMSERVER UNI 232/422/485"]
[null,null,null,"2-Port","EKI-1222\nEKI-1222D","MGate MB3280\nMGate MB3270","PortServer TS 2 MEI","N/A","N/A"]
[null,null,null,"4-Port","EKI-1224","MGate MB3480 ","PortServer TS 4 MEI","N/A","N/A"]
[null,"USB Converters",null,null,"USB-4604B","UPort 2410\nUPort 1410","Edgeport® Industrial /4","N/A","N/A"]
[null,null,null,null,"USB-4604BM","UPort 1450","Edgeport® Industrial /4","N/A","N/A"]

{"sheet":"DS - Managed Switch","index":10,"n_rows":91,"n_cols":34,"rows_kept":91,"cut":false,"hidden":false,"merged":[[82,0,82,15],[0,1,0,5],[72,0,72,15],[0,6,0,9],[0,28,0,33]]}
[null,"EKI-2000 Series",null,null,null,null,"EKI-7000 Series",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EKI-9000Series"]
[null,"EKI-2548I","EKI-2548SI","EKI-2548MI","EKI-2748CI","EKI-2748FI","EKI-7554SI","EKI-7554MI","EKI-7556MI","EKI-7559SI","EKI-7559MI","EKI-7654C","EKI-7656C/CI","EKI-7657C","EKI-7659C/CI","EKI-7758F","EKI-7710E-2C","EKI-7710E-2CI","EKI-7710G-2C","EKI-7710G-2CI","EKI-7712G-4F-AE","EKI-7712G-4FI-AE","EKI-7712E-4F-AE","EKI-7712E-4FI-AE","EKI-7720G-4F-AE","EKI-7720G-4FI-AE","EKI-7720E-4F-AE","EKI-7720E-4FI-AE","EKI-9316P","EKI-9316","EKI-9312P","EKI-9312","EKI-9228G-8CMI","EKI-9228G-8COI"]
["Switch Classification"]
["Web Managed-Smart Grade","●","●","●","●","●",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●","●"]
["Layer 2",null,null,null,null,null,"●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Connectivity"]
["10/100Base-TX, Fixed",8,6,6,null,null,4,4,16,8,8,4,16,7,8,null,"8","8",null,null,null,null,"8","8",null,null,"16","16"]
["10/100/1000Based-T,Fixed",null,null,null,6,4,null,null,null,null,null,null,null,null,null,4,null,null,"8","8","8","8",null,null,"16","16",null,null,12,12,8,8,"16","16"]
["Combo \n(Fixed RJ45 1000Base-Tx or SFP)",null,null,null,2,null,null,null,null,null,null,2,2,3,2,null,"2","2","2","2",null,null,null,null,null,null,null,null,null,null,null,null,"8","8"]
["100FX Fiber, Fixed",null,2,2,null,null,2,2,2,2,2]
["100FX Fiber mode",null,"Single-mode","Multi-mode",null,null,"Single-mode","Multi-mode","Multi-mode","Single-mode","Multi-mode"]
["100FX Fiber connector type",null,"SC ","SC",null,null,"SC ","SC","SC","SC ","SC"]
["Open SFP Slot (GbE)",null,null,null,null,4,null,null,null,null,null,null,null,null,null,4,null,null,null,null,"4","4","4","4","4","4","4","4",4,4,4,4,"4","4"]
["Open SFP Slot (Compatibility 100-FX)",null,null,null,"●","●",null,null,null,null,null,"●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Open SFP+ Slot (10 GbE)"]
["Performance"]
["Switch Fabric Speed,Gbps","1.6Gbps","1.6Gbps","1.6Gbps","16Gbps","16Gbps","1.2Gbps","1.2Gbps","3.6Gbps","2Gbps","2Gbps","4.8Gbps","7.2Gbps","7.4Gbps","5.6Gbps","16Gbps","5.6Gbps","5.6Gbps","20Gbps","20Gbps","24Gbit","24Gbit","9.6Gbit","9.6Gbit","40Gbit","40Gbit","11.2Gbit","11.2Gbit","32Gb","32Gb","24Gb","24Gb","56Gbps","56Gbps"]
["Packet buffer,Bytes","128KB","128KB","128KB","128KB","128KB","128KB","128KB","128KB","128KB","128KB","128KB","128KB","128KB","128KB","128KB","4.1Mb","4.1Mb","4.1Mb","4.1Mb","4.1Mb","4.1Mb","4.1Mb","4.1Mb","4.1Mb","4.1Mb","4.1Mb","4.1Mb","1.5MB","1.5MB","1.5MB","1.5MB","1.5MB","1.5MB"]
["Jumbo Frame","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","9216Bytes","9216Bytes","9216Bytes","9216Bytes","9216Bytes","9216Bytes","9216Bytes","9216Bytes","9216Bytes","9216Bytes","9216Bytes","9216Bytes","12kb","12kb","12kb","12kb","9216Bytes","9216Bytes"]
["MAC Address Table","2K","2K","2K","8K","8K","8K","8K","8K","8K","8K","8k","8k","8k","8k","8k","8k","8k","8k","8k","8k","8k","8k","8k","8k","8k","8k","8k","16k","16k","16k","16k","16k","16k"]
["HW Watch Dog Supported","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","●","●","●","●","●","●","●","●","●","●","●","●"]
["MTBF","215,266 hrs","337,238 hrs","337,238 hrs","248,507hrs","289,385 hrs","264,964hrs","264,964hrs","218,490hrs","262,230hrs","262,230hrs","294,410hrs","220,111hrs","250,472hrs","249,547hrs","289,385 hrs","858,835 hrs","858,835 hrs","858,835 hrs","858,835 hrs",null,null,null,null,null,null,null,null,"848,749 hrs","1,177,031 hrs","851,847 hrs","1,180,639 hrs"]
["Physical"]
["Dimensions ( WxHxD )","59.6x152x105 mm","59.6x152x105 mm","59.6x152x105 mm","59.6x152x105 mm","59.6x152x105 mm","79x152x105 mm","79x152x105 mm","79x152x105 mm","79x152x105 mm","79x152x105 mm","79x152x105 mm","79x152x105 mm","79x152x105 mm","79x152x105 mm","79x152x105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","305x215x120 mm","305x215x120 mm","305x215x120 mm","305x215x120 mm","442 x 44 x 352","442 x 44 x 352"]
["Rack Size","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["Power"]
["Power Input Voltage","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","48VDC","24~48VDC","48VDC","24~48VDC","48VDC","90~264AC/88~370VDC"]
["Dual Power Input","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Relay Output","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Power Consumption(Max, 48VDC)","7.6 Watts","10.6 Watts","10.6 Watts","15.5 Watts","13 Watts","8.4 Watts","8.4 Watts","10.8 Watts","11.3 Watts","11.3 Watts","7 Watts","11.5 Watts","10.7 Watts","9.5 Watts","13 Watts","12.1 Watts","12.1 Watts","12.1 Watts","12.1 Watts","12.1 Watts","12.1 Watts","12.1 Watts","12.1 Watts",null,null,null,null,"295 Watts","22 Watts","204 Watts","22 Watts","19.24 Watts","19.24 Watts"]
["Power Consumption(Max, 220VAC)"]
["Input Reverse Protection","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["L2 Feature"]
["IEEE 802.3x Flow Control ","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Static/802.3ad LACP (Link Aggregation Control Protocol)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["VLAN, Max. VLAN Supported",256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,"4K","4K","4K","4K","256","256"]
["Available VLAN ID Range","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094"]
["Port-Based VLAN ","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["802.1Q VLAN Trunking ","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["802.1ad VLAN Stacking (QinQ) ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["GVRP (Generic VLAN Registration Protocol)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["GARP (Generic Attribute Registration Protocol)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Max Multicast Group Supported ","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["IGMP Snooping (v1,v2)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["IGMP Querier","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["IGMP Filtering ","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","-","-","-","-","-","-"]
["Redudancy"]
["IEEE 802.1D (STP)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["IEEE 802.1w (RSTP)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["X-Ring (Advantech Propietary)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Security"]
["802.1x (Port-Based)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Port Security ","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Layer 2 MAC filtering ","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Quality of Service (QoS)"]
["802.1p Priority Queues per Port ",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,"8","8","8","8","8","8","8","8","8","8","8","8",8,8,8,8,8,8]
["802.1p Queuing method ","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SP/WRR/Hybrid Priority","SP/WRR/Hybrid Priority","SP/WRR/Hybrid Priority","SP/WRR/Hybrid Priority","SP/WRR/Hybrid Priority","SP/WRR/Hybrid Priority"]
["Class of Service (CoS)"]
["802.1p based COS","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["IP TOS/Precedence based COS","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["DSCP based COS","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["TCP/UDP Port based COS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-","-","-"]
["Management"]
["CLI","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Web Based Management","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Telnet Management","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Console Management","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["SNMP(v1,v2c)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Backup/Restore(TFTP,HTTP)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["DNS",null,null,null,"●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["DHCP Server",null,null,null,"●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["DHCP Client","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Diagnostic"]
["Port Mirror","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["SNMP(v1,v2c)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["RMON(1,2,3,9 Group)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["SNTP","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Event/Error Log(Local Flash)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Real-Time Traffic Statistic","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["SNMP Trap","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Email Alert","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["DI/DO",null,null,null,null,null,null,null,null,null,null,null,null,"●",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-","-","-","-","-","-"]
["Certification"]
["UL60950-1",null,null,null,null,null,"●","●",null,"●","●","●","●","●","●","●",null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●","●"]
["UL508","●","●","●","●","●","●(BE version)",null,"●",null,"●(BE version)",null,null,null,null,null,"●","●","●","●"]
["UL61010",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●","●","●","●","●","●",null,null,null,null,"●","●"]
["UL-C1D2","●","●","●","●","●",null,null,null,"●","●",null,"●","●",null,"●",null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●","●"]
["3C","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●",null,null,null,null,null,null,null,null,null,null,null,null,"-","-","-","-"]
["FCC","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["CE","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Others",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2",null,null,null,null,"IEC-61850-3","IEC-61850-3"]

{"sheet":"DS - Lite Managed Switch ","index":11,"n_rows":90,"n_cols":25,"rows_kept":90,"cut":false,"hidden":false,"merged":[[72,0,72,8],[0,1,0,8],[0,9,0,16],[0,17,0,24],[82,0,82,24]]}
[null,"EtherNet/IP series",null,null,null,null,null,null,null,"Modbus/TCP Series",null,null,null,null,null,null,null,"PROFINET Series"]
[null,"EKI-5528-EI","EKI-5528I-EI","EKI-5526-EI","EKI-5526I-EI","EKI-5629C-EI","EKI-5629CI-EI","EKI-5626C-EI","EKI-5626CI-EI","EKI-5528-MB","EKI-5528I-MB","EKI-5526-MB","EKI-5526I-MB","EKI-5629C-MB","EKI-5629CI-MB","EKI-5626C-MB","EKI-5626CI-MB","EKI-5528-PN","EKI-5528I-PN","EKI-5526-PN","EKI-5526I-PN","EKI-5629C-PN","EKI-5629CI-PN","EKI-5626C-PN","EKI-5626CI-PN"]
["Switch Classification"]
["Web Managed-Smart Grade"]
["Layer 2"]
["Connectivity"]
["10/100Base-TX, Fixed",8,"8","16","16","8","8","16","16",8,"8","16","16","8","8","16","16",8,"8","16","16","8","8","16","16"]
["10/100/1000Based-T,Fixed"]
["Combo \n(Fixed RJ45 1000Base-Tx or SFP)",null,null,null,null,"2","2","2","2",null,null,null,null,"2","2","2","2",null,null,null,null,"2","2","2","2"]
["100FX Fiber, Fixed"]
["100FX Fiber mode"]
["100FX Fiber connector type"]
["Open SFP Slot (GbE)"]
["Open SFP Slot (Compatibility 100-FX)"]
["Open SFP+ Slot (10 GbE)"]
["Performance"]
["Switch Fabric Speed,Gbps","1.6Gbps","1.6Gbps","3.2Gbps","3.2Gbps","5.6Gbps","5.6Gbps","7.2Gbps","7.2Gbps","1.6Gbps","1.6Gbps","3.2Gbps","3.2Gbps","5.6Gbps","5.6Gbps","7.2Gbps","7.2Gbps","1.6Gbps","1.6Gbps","3.2Gbps","3.2Gbps","5.6Gbps","5.6Gbps","7.2Gbps","7.2Gbps"]
["Packet buffer,Bytes","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit"]
["Jumbo Frame","-","-","-","-",null,null,"-",null,"-","-","-","-",null,null,"-",null,"-","-","-","-",null,null,"-"]
["MAC Address Table","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry"]
["HW Watch Dog Supported","-","-","-","-",null,null,"-",null,"-","-","-","-",null,null,"-",null,"-","-","-","-",null,null,"-"]
["MTBF","4,176,861 hours","4,176,861 hours","2,788,343 hours","2,788,343 hours","3,183,604 hours","3,183,604 hours","2,825,281 hours","2,825,281 hours","4,176,861 hours","4,176,861 hours","2,788,343 hours","2,788,343 hours","3,183,604 hours","3,183,604 hours","2,825,281 hours","2,825,281 hours","4,176,861 hours","4,176,861 hours","2,788,343 hours","2,788,343 hours","3,183,604 hours","3,183,604 hours","2,825,281 hours","2,825,281 hours"]
["Physical"]
["Dimensions ( WxHxD )","43 x 120 x 84 mm","43 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","43 x 120 x 84 mm","43 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","43 x 120 x 84 mm","43 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm"]
["Rack Size","-","-","-","-",null,null,"-",null,"-","-","-","-",null,null,"-",null,"-","-","-","-",null,null,"-"]
["Power"]
["Power Input Voltage","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC"]
["Dual Power Input","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Relay Output","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Power Consumption(Max, 48VDC)","5.2 Watts","5.2 Watts","8 Watts","8 Watts","5.8 Watts","5.8 Watts","8.2 Watts","8.2 Watts","5.2 Watts","5.2 Watts","8 Watts","8 Watts","5.8 Watts","5.8 Watts","8.2 Watts","8.2 Watts","5.2 Watts","5.2 Watts","8 Watts","8 Watts","5.8 Watts","5.8 Watts","8.2 Watts","8.2 Watts"]
["Power Consumption(Max, 220VAC)"]
["Input Reverse Protection","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["L2 Feature"]
["IEEE 802.3x Flow Control ","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Static/802.3ad LACP (Link Aggregation Control Protocol)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["VLAN, Max. VLAN Supported",256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256]
["Available VLAN ID Range","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094"]
["Port-Based VLAN ","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["802.1Q VLAN Trunking ","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["802.1ad VLAN Stacking (QinQ) "]
["GVRP (Generic VLAN Registration Protocol)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["GARP (Generic Attribute Registration Protocol)"]
["Max Multicast Group Supported ","●","●","●","●",null,null,"●",null,"●","●","●","●",null,null,"●",null,"●","●","●","●",null,null,"●"]
["IGMP Snooping (v1,v2)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["IGMP Querier","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["IGMP Filtering ","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Redudancy"]
["IEEE 802.1D (STP)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["IEEE 802.1w (RSTP)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["X-Ring (Advantech Propietary)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Security"]
["802.1x (Port-Based)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Port Security ","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Layer 2 MAC filtering ","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Quality of Service (QoS)"]
["802.1p Priority Queues per Port ",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["802.1p Queuing method ","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR"]
["Class of Service (CoS)"]
["802.1p based COS","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["IP TOS/Precedence based COS","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["DSCP based COS","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["TCP/UDP Port based COS"]
["Management"]
["CLI"]
["Web Based Management","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Telnet Management"]
["Console Management"]
["SNMP(v1,v2c)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Backup/Restore(TFTP,HTTP)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["DNS","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["DHCP Server"]
["DHCP Client","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Diagnostic"]
["Port Mirror","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["SNMP(v1,v2c)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["RMON(1,2,3,9 Group)"]
["SNTP","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Event/Error Log(Local Flash)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Real-Time Traffic Statistic","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["SNMP Trap","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Email Alert"]
["DI/DO"]
["Certification"]
["UL60950-1"]
["UL508","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["UL-C1D2","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["3C"]
["FCC","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["CE","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Others","EtherNet/IP ","EtherNet/IP ","EtherNet/IP ","EtherNet/IP ","EtherNet/IP ","EtherNet/IP ","EtherNet/IP ","EtherNet/IP ",null,null,null,null,null,null,null,null,"PROFINET","PROFINET","PROFINET","PROFINET","PROFINET","PROFINET","PROFINET","PROFINET"]

{"sheet":"DS - Proview Switch","index":12,"n_rows":50,"n_cols":41,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[null,"EKI-5525S-AE","EKI-5525SI-AE","EKI-5525M-AE","EKI-5525MI-AE","EKI-5525S-ST-AE","EKI-5525SI-ST-AE","EKI-5525M-ST-AE","EKI-5525MI-ST-AE","EKI-5524SS-AE","EKI-5524SSI-AE","EKI-5524MM-AE","EKI-5524MMI-AE","EKI-5524SS-ST-AE","EKI-5524SSI-ST-AE","EKI-5524MM-ST-AE","EKI-5524MMI-ST-AE","EKI-5525-AE","EKI-5525I-AE","EKI-5725-AE","EKI-5725I-AE","EKI-5728-AE","EKI-5728I-AE","EKI-5729F-AE","EKI-5729FI-AE","EKI-5528-AE","EKI-5528I-AE","EKI-5526-AE","EKI-5526I-AE","EKI-5726-AE","EKI-5726I-AE","EKI-5726F-AE","EKI-5726FI-AE","EKI-5629C-AE","EKI-5629CI-AE","EKI-5626C-AE","EKI-5626CI-AE","EKI-5624P-AE","EKI-5624PI-AE","EKI-5729P-AE","EKI-5729PI-AE"]
["Connectivity"]
["10/100Base-Tx, fixed",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,5,5,null,null,null,null,null,null,8,8,16,16,null,null,null,null,8,8,16,16]
["10/100Base-TX PoE, fixed",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,4]
["10/100/1000Based-Tx,fixed",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,5,8,8,8,8,null,null,null,null,16,16,16,16,null,null,null,null,2,2,2,2]
["10/100/1000Base-T PoE, fixed",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,8]
["Combo \n(Fixed RJ45 1000Base-Tx or SFP)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,2,2,2]
["100FX Fiber, fixed",1,1,1,1,1,1,1,1,2,2,2,2,2,2,2,2]
["100FX Fiber mode","Single-Mode","Single-Mode","Multi-Mode","Multi-Mode","Single-Mode","Single-Mode","Multi-Mode","Multi-Mode","Single-Mode","Single-Mode","Multi-Mode","Multi-Mode","Single-Mode","Single-Mode","Multi-Mode","Multi-Mode"]
["100FX Fiber connector type","SC","SC","SC","SC","ST","ST","ST","ST","SC","SC","SC","SC","ST","ST","ST","ST"]
["Open SFP slot (GbE)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,2,null,null,null,null,null,null,2,2]
["Open SFP Slot (Compatibility 100-FX)"]
["Auto MDI/MDI-X","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Auto Negotiation","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Performance"]
["Switch fabric speed,Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","1Gbps","10Gbps","10Gbps","16Gbps","16Gbps","20Gbps","20Gbps","1.6Gbps","1.6Gbps","3.2Gbps","3.2Gbps","32Gbps","32Gbps","36Gbps","36Gbps","5.6Gbps","5.6Gbps","7.2Gbps","7.2Gbps","4.8Gbps","4.8Gbps","5.6Gbps","5.6Gbps"]
["IEEE 802.3az","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes","Yes"]
["Throughput, Mpps"]
["Packet buffer","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","1Mbits","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","TBC","TBC","TBC","TBC","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1 Mbit","4.1M bit","4.1M bit","4.1M bit","4.1M bit","1M bit","1M bit","4.1M bit","4.1M bit"]
["MAC address table","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","2K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","8K-entry","2K-entry","2K-entry","8K-entry","8K-entry"]
["MTBF","282,703 hours","282,703 hours","282,703 hours","282,703 hours","282,703 hours","282,703 hours","282,703 hours","282,703 hours","144,890 hours","144,890 hours","144,890 hours","144,890 hours","144,890 hours","144,890 hours","144,890 hours","144,890 hours","5,168,110 hours","5,168,110 hours","5,168,110 hours","5,168,110 hours","4,176,861 hours","4,176,861 hours","3,858,286 hours","3,858,286 hours","5,235,270 hours","5,235,270 hours","4,653,552 hours","4,653,552 hours","2,788,343 hours","2,788,343 hours","1,962,789 hours","1,962,789 hours","3,183,604 hours","3,183,604 hours","2,825,281 hours","2,825,281 hours","TBD","TBD","TBD","TBD"]
["Heat Dissipation"]
["Traffic Control"]
["Broadcast Storm protection"]
["Jumbo frame size","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","2048-byte","2048-byte","2048-byte","2048-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte","9216-byte"]
["IEEE 802.3x flow control","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Loop Detection","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Physical"]
["Housing Dimensions \n(  WxHxD ) mm","27 x 120 x 84 mm ","27 x 120 x 84 mm ","27 x 120 x 84 mm ","27 x 120 x 84 mm ","27 x 120 x 84 mm ","27 x 120 x 84 mm ","27 x 120 x 84 mm ","27 x 120 x 84 mm ","43 x 120 x 84 mm","43 x 120 x 84 mm","43 x 120 x 84 mm","43 x 120 x 84 mm","43 x 120 x 84 mm","43 x 120 x 84 mm","43 x 120 x 84 mm","43 x 120 x 84 mm","27 x 120 x 84 mm ","27 x 120 x 84 mm ","27 x 120 x 84 mm ","27 x 120 x 84 mm ","43 x 120 x 84 mm","43 x 120 x 84 mm","43 x 120 x 84 mm","43 x 120 x 84 mm","43 x 120 x 84 mm","43 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 120 x 84 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm"]
["PCBA Size(WxD mm)"]
["Mounting way","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount"]
["IP rating","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30"]
["Power"]
["Power Input voltage","12~48VDC ","12~48VDC ","12~48VDC ","12~48VDC ","12~48VDC ","12~48VDC ","12~48VDC ","12~48VDC ","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V ","12V~48V ","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V","12V~48V ","12V~48V ","12V~48V ","12VDC~24VDC","12VDC~24VDC","12VDC~24VDC","12VDC~24VDC"]
["Dual Power input","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Relay output","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Power Consumption","2.8 W","2.8 W","2.8 W","2.8 W","2.8 W","2.8 W","2.8 W","2.8 W","4 W","4 W","4 W","4 W","4 W","4 W","4 W","4 W","2 W","2 W","2 W","2 W","5.2 W","5.2 W","6.8 W","6.8 W","3.6 W","3.6 W","3.84 W","3.84 W","8 W","8 W","9.6 W","9.6 W","5.8 W","5.8 W","8.2 W","8.2 W","60 W","60 W","65 W","65 W"]
["Reverse protection","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Certification"]
["IEC/EN 60950-1","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["UL508","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["UL61010-1+UL61010-2-201",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●","●"]
["UL-C1D2","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["3C"]
["FCC","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["CE","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["e-Mark",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●","●",null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●","●"]
["ATEX","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["IECEx","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["DNV (compliant)"]

{"sheet":"DS - Unmanaged Switch","index":13,"n_rows":45,"n_cols":25,"rows_kept":45,"cut":false,"hidden":false,"merged":[[0,17,0,18],[0,19,0,24],[0,13,0,16],[0,1,0,12]]}
[null,"EKI-2000 Series",null,null,null,null,null,null,null,null,null,null,null,"EKI-3000 Series",null,null,null,"EKI-4000 Series",null,"EKI-7000 Series"]
[null,"EKI-2525/I","EKI-2525M","EKI-2525M-ST","EKI-2526M","EKI-2526S","EKI-2526M-ST","EKI-2526S-ST","EKI-2528/I","EKI-2725","EKI-2728/I","EKI-2728MI","EKI-2701PSI","EKI-3525","EKI-3528","EKI-3725","EKI-3728","EKI-4524RI","EKI-4524I","EKI-7526I","EKI-7526MI","EKI-7529MI","EKI-7529MI-ST","EKI-7626C/CI","EKI-7629C/CI"]
["Connectivity"]
["10/100Base-Tx, fixed",5,4,4,4,4,4,4,8,null,null,null,null,5,8,null,null,24,24,16,16,8,8,16,8]
["10/100Base-TX PoE, fixed"]
["10/100/1000Based-Tx,fixed",null,null,null,null,null,null,null,null,5,8,6,1,null,null,5,8]
["10/100/1000Base-T PoE, fixed"]
["Combo \n(Fixed RJ45 1000Base-Tx or SFP)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,2]
["100FX Fiber, fixed",null,1,1,2,2,2,2,null,null,null,"2 (Gigabit)",null,null,null,null,null,null,null,null,2,2,2]
["100FX Fiber mode",null,"Multi-mode","Multi-mode","Multi-mode","Single-mode","Multi-mode","Single-mode",null,null,null,"Multi-mode",null,null,null,null,null,null,null,null,"Multi-mode","Multi-mode","Multi-mode"]
["100FX Fiber connector type",null,"SC","ST","SC","SC","ST","ST",null,null,null,"SC",null,null,null,null,null,null,null,null,"SC","SC","ST"]
["Open SFP slot (GbE)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2]
["Open SFP Slot (Compatibility 100-FX)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●"]
["Auto MDI/MDI-X","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Auto Negotiation","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Performance"]
["Switch fabric speed,Gbps","1.0Gbps","1.0Gbps","1.0Gbps","1.0Gbps","1.0Gbps","1.2Gbps","1.2Gbps","1.6Gbps","10Gbps","16Gbps","16Gbps","-","1.0Gbps","1.6Gbps","10Gbps","16Gbps","5.2Gbps","4.8 Gbps","3.2Gbps","3.6Gbps","2Gbps","2Gbps","7.2Gbps","5.6Gbps"]
["IEEE 802.3az",null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Yes","Yes","Yes"]
["Throughput, Mpps","1.4881Mpps","1.4881Mpps","1.4881Mpps","1.4881Mpps","1.4881Mpps","1.78572Mpps","1.78572Mpps","2.38096Mpps","14.88095Mpps","23.80952Mpps","23.80952Mpps","-","148809PKs/SEC","148809PKs/SEC","1488095PKs/SEC","1488095PKs/SEC","7.73812Mpps","7.14286Mpps","4.76192Mpps","5.35716Mpps","2.9762Mpps","2.9762Mpps","10.7143Mpps","8.33334Mpps"]
["Packet buffer","56KB","56KB","56KB","56KB","56KB","56KB","56KB","56KB","17KB","192KB","176KB","-","384k bits","768k bits","1M bits","1M bits","512KB","256KB","128KB","128KB","128KB","128KB","128KB","128KB"]
["MAC address table","2K","2K","2K","2K","2K","2K","2K","2K","8K","4K","48-bit","-","2K-entry","2K-entry","2K-entry","8K-entry","8K","8K","8K","8K","8K","8K","8K","8K"]
["MTBF","402,589hrs","674,572hrs","674,572hrs","359,411hrs","359,411hrs","359,411hrs","359,411hrs","388,566hrs","627,957hrs","589,289hrs","505,863hrs","1,419,817hrs","1,567,102Hrs"," 1,516,457Hrs","1,545,555 Hrs","1,478,582Hrs","193,177hrs","174,736hrs","261,542hrs","237,130hrs","289,518hrs","289,518hrs","307,177hrs","295,662hrs"]
["Traffic Control"]
["Broadcast Storm protection","●","●","●","●","●","●","●","●","●","●","●","●","Yes","Yes","Yes","Yes","●","●","●","●","●","●","●","●"]
["Jumbo frame size",null,null,null,null,null,null,null,null,"9026bytes","9720bytes","9026bytes",null,"NO support","NO support","9216 Byte","9216 Byte"]
["IEEE 802.3x flow control","●","●","●","●","●","●","●","●","●","●","●","●","Yes","Yes","Yes","Yes","●","●","●","●","●","●","●","●"]
["Loop Detection",null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●","●"]
["Physical"]
["Housing Dimensions \n(  WxHxD ) mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","28.5 x 120 x 85.3 mm ","44.5 x 120 x 85.3 mm ","28.5 x 120 x 85.3 mm ","44.5 x 120 x 85.3 mm ","440x44x280 mm","440x44x224 mm","79x152x105 mm","79x152x105 mm","79x152x105 mm","79x152x105 mm","79x152x105 mm","79x152x105 mm"]
["Mounting way","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","Rack-mount","Rack-mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount"]
["IP rating","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP40","IP40","IP40","IP40","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30"]
["Power"]
["Power Input voltage","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","44~57VDC","8.4~52.4VDC","8.4~52.4VDC","8.4~52.4VDC","8.4~52.4VDC","100~240VAC/VDC","100~240VAC/VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC"]
["Dual Power input","●","●","●","●","●","●","●","●","●","●","●",null,"●","●","●","●","●","●","●","●","●","●","●","●"]
["Relay output","●","●","●","●","●","●","●","●","●","●","●",null,"●","●","●","●","●","●","●","●","●","●","●","●"]
["Power Consumption","2.88 Watts","4.2 Watts","4.2 Watts","58 Watts","58 Watts","6.4 Watts","6.4 Watts","3.9 Watts","4.6 Watts","5.3 Watts","9.3 Watts","17.8 Watts","2 Watts","2.1 Watts","2.14 Watts","4.5 Watts","13.9 Watts","14.5 Watts","5.28 Watts","8.9 Watts","6.7 Watts","6.7 Watts","9 Watts","6.8 Watts"]
["Reverse protection","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Certification"]
["UL60950-1","●","●","●","●","●","●","●","●","●","●",null,"●","●","●","●","●",null,null,null,null,null,null,"●","●"]
["UL508",null,null,null,null,null,null,null,null,null,null,"●",null,null,null,null,null,null,null,"●","●","●","●"]
["UL61010"]
["UL-C1D2","●","●",null,"●","●",null,null,"●",null,"●"]
["3C","●","●","●","●","●","●","●","●","●","●","●","●",null,null,null,null,"●","●","●","●","●","●","●","●"]
["FCC","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["CE","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]

{"sheet":"DS - PoE  Switch","index":14,"n_rows":88,"n_cols":23,"rows_kept":88,"cut":false,"hidden":false,"merged":[[69,0,69,1],[79,0,79,1],[0,1,0,7],[0,11,0,22]]}
[null,"Managed PoE Switch",null,null,null,null,null,null,null,null,null,"Unmanaged PoE Switch"]
[null,"EKI-7659CPI","EKI-7710E-2CP","EKI-7710E-2CPI","EKI-7710G-2CP","EKI-7710G-2CPI","EKI-7712G-2CP","EKI-7712G-2CPI",null,null,"EKI-3725P","EKI-2525P","EKI-2525PA","EKI-2525SPI","EKI-2526PI","EKI-2528PAI","EKI-2726FHPI","EKI-2701HPI","EKI-7629CP/I","EKI-2706E-1GFP","EKI-2706E-1GFPI","EKI-2706G-1GFP","EKI-2706G-1GFPI"]
["Connectivity",null,null,null,null,null,null,null,null,"Connectivity"]
["10/100Base-TX, Fixed",null,null,null,null,null,null,null,null,"10/100Base-Tx, fixed",null,1,1,null,2,4]
["10/100Base-TX PoE, Fixed",8,8,8,null,null,null,null,null,"10/100Base-TX PoE, fixed",null,4,4,4,4,4,null,null,8,4,4]
["10/100/1000Based-T,Fixed",null,null,null,8,8,null,null,null,"10/100/1000Based-Tx,fixed",1,null,null,null,null,null,null,1,null,1,1,1,1]
["10/100/1000Base-T PoE, Fixed",null,null,null,null,null,8,8,null,"10/100/1000Base-T PoE, fixed",4,null,null,null,null,null,"4 (802.3at)","1 (802.3at)",null,null,null,4,4]
["Combo \n(Fixed RJ45 1000Base-Tx or SFP)",2,2,2,2,2,null,null,null,"Combo \n(Fixed RJ45 1000Base-Tx or SFP)",null,null,null,null,null,null,null,null,2]
["100FX Fiber, Fixed",null,null,null,null,null,null,null,null,"100FX Fiber, fixed",null,null,null,1]
["100FX Fiber mode",null,null,null,null,null,null,null,null,"100FX Fiber mode",null,null,null,"Single-mode"]
["100FX Fiber connector type",null,null,null,null,null,null,null,null,"100FX Fiber connector type",null,null,null,"SC"]
["Open SFP Slot (GbE)",null,null,null,null,null,4,4,null,"Open SFP slot (GbE)",null,null,null,null,null,null,null,null,null,1,1,1,1]
["Open SFP Slot (Compatibility 100-FX)","●","●","●","●","●","●","●",null,"Open SFP Slot (Compatibility 100-FX)",null,null,null,null,null,null,2,null,"●"]
["Performance",null,null,null,null,null,null,null,null,"Performance"]
["Switch Fabric Speed,Gbps","5.6Gbps","5.6Gbps","5.6Gbps","20Gbps","20Gbps","24Gbps","24Gbps",null,"Switch fabric speed,Gbps","5Gbps","1.0Gbps","1.0Gbps","1.0Gbps","1.2Gbps","1.6Gbps","12Gbps","4Gbps","5.6Gbps","4.8Gbps","4.8Gbps","12Gbps","12Gbps"]
["Packet buffer,Bytes","128KB","4.1Mb","4.1Mb","4.1Mb","4.1Mb","4.1Mb","4.1Mb",null,"IEEE 802.3az","Yes"]
["MAC Address Table","8k","8k","8k","8k","8k","8k","8k",null,"Packet buffer","1M bit","56KB","56KB","56KB","56KB","56KB","1M bits","-","128KB","4.1Mb","4.1Mb","4.1Mb","4.1Mb"]
["HW Watch Dog Supported","-","●","●","●","●","●","●",null,"MAC address table","2K-entry","2K","2K","2K","2K","2K","4K-entry","-","8K","2K","2K","2K","2K"]
["MTBF","181,652hrs","858,835 hrs","858,835 hrs","858,835 hrs","858,835 hrs",null,null,null,"MTBF","434,533Hrs","443,153hrs","196,813hrs","421,106hrs","210,323hrs","241,413hrs","339,740 Hrs","1,478,582Hrs","267,793hrs"]
["Physical",null,null,null,null,null,null,null,null,"Physical"]
["Dimensions ( WxHxD )","79x152x105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm","74 x 152 x 105 mm",null,"Housing Dimensions (WxHxD) mm","25.6 x 120 x 83 mm","37x140x95 mm","48.6x140x95 mm","37x140x95 mm","48.6x140x95 mm","48.6x140x95 mm","59.6 x 152 x 105 mm","37 x 140 x 95 mm","79x152x105 mm","30 x 140 x 95","30 x 140 x 95","30 x 140 x 95","30 x 140 x 95"]
["Mounting way","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount","DIN-Rail and Wall mount",null,"Mounting way","DIN-Rail and Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount"]
["IP rating","IP40","IP30","IP30","IP30","IP30","IP30","IP30",null,"IP rating","IP40","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30"]
["Power",null,null,null,null,null,null,null,null,"Power"]
["Power Input Voltage","12~48VDC","24~48VDC","24~48VDC","24~48VDC","24~48VDC",null,null,null,"Power Input voltage","24V~48V","48VDC","24~48VDC","48VDC","48VDC","24~48VDC","48 VDC(44VDC to 57 VDC) ","24~48VDC","48VDC","48VDC","48VDC","48VDC","48VDC"]
["Dual Power Input","●","●","●","●","●","●","●",null,"Dual Power input","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Relay Output","●","●","●","●","●","●","●",null,"Relay output","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Power Consumption(Max, 48VDC)","142 Watts","132 Watts","132 Watts","132 Watts","132 Watts","252.1 Watts","252.1 Watts",null,"Power Consumption","61.6 Watts","57 Watts","62.5W","58 Watts","62.5 Watts","72 Watts","130 Watts","33.4 Watts","116 Watts","2 Watts","2 Watts","2 Watts","2 Watts"]
["Input Reverse Protection","●","●","●","●","●","●","●",null,"Reverse protection","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["L2 Feature",null,null,null,null,null,null,null,null,"Traffic Control"]
["IEEE 802.3x Flow Control ","●","●","●","●","●","●","●",null,"Broadcast Storm protection",null,"●","●","●","●","●","-","-","●","●","●","●","●"]
["Static/802.3ad LACP (Link Aggregation Control Protocol)","●","●","●","●","●","●","●",null,"Jumbo frame size","9216 Bytes",null,null,null,null,null,"-","-",null,"9216 Bytes","9216 Bytes","9216 Bytes","9216 Bytes"]
["VLAN, Max. VLAN Supported",256,256,256,256,256,256,256,null,"IEEE 802.3x flow control","●","●","●","●","●","●","Yes","Yes","●","●","●","●","●"]
["Available VLAN ID Range","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094",null,"Certification"]
["Port-Based VLAN ","●","●","●","●","●","●","●",null,"UL60950-1","●","●",null,"●",null,null,null,null,"●"]
["802.1Q VLAN Trunking ","●","●","●","●","●","●","●",null,"UL508",null,null,"●",null,null,"●","●","●"]
["802.1ad VLAN Stacking (QinQ) ",null,"●","●","●","●","●","●",null,"UL61010",null,null,null,null,null,null,null,null,null,"●","●","●","●"]
["GVRP (Generic VLAN Registration Protocol)","●","●","●","●","●","●","●",null,"UL-C1D2"]
["GARP (Generic Attribute Registration Protocol)",null,"●","●","●","●","●","●",null,"3C",null,"●","●","●","●","●"]
["Max Multicast Group Supported ","●","●","●","●","●","●","●",null,"FCC","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["IGMP Snooping (v1,v2)","●","●","●","●","●","●","●",null,"CE","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["IGMP Querier","●","●","●","●","●","●","●"]
["IGMP Filtering ","●","●","●","●","●","●","●"]
["Redudancy"]
["IEEE 802.1D (STP)","●","●","●","●","●","●","●"]
["IEEE 802.1w (RSTP)","●","●","●","●","●","●","●"]
["X-Ring (Advantech Propietary)","●","●","●","●","●","●","●"]
["Security"]
["802.1x (Port-Based)","●","●","●","●","●","●","●"]
["Port Security ","●","●","●","●","●","●","●"]
["Layer 2 MAC filtering ","●","●","●","●","●","●","●"]
["Quality of Service (QoS)"]
["802.1p Priority Queues per Port ",4,8,8,8,8,8,8]
["802.1p Queuing method ","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR"]
["Class of Service (CoS)"]
["802.1p based COS","●","●","●","●","●","●","●"]
["IP TOS/Precedence based COS","●","●","●","●","●","●","●"]
["DSCP based COS","●","●","●","●","●","●","●"]
["TCP/UDP Port based COS"]
["Management"]
["CLI","●","●","●","●","●","●","●"]
["Web Based Management","●","●","●","●","●","●","●"]
["Telnet Management","●","●","●","●","●","●","●"]
["Console Management","●","●","●","●","●","●","●"]
["SNMP(v1,v2c)","●","●","●","●","●","●","●"]
["Backup/Restore(TFTP,HTTP)","●","●","●","●","●","●","●"]
["DNS","●","●","●","●","●","●","●"]
["DHCP Server","●","●","●","●","●","●","●"]
["DHCP Client","●","●","●","●","●","●","●"]
["Diagnostic"]
["Port Mirror","●","●","●","●","●","●","●"]
["SNMP(v1,v2c)","●","●","●","●","●","●","●"]
["RMON(1,2,3,9 Group)","●","●","●","●","●","●","●"]
["SNTP","●","●","●","●","●","●","●"]
["Event/Error Log(Local Flash)","●","●","●","●","●","●","●"]
["Real-Time Traffic Statistic","●","●","●","●","●","●","●"]
["SNMP Trap","●","●","●","●","●","●","●"]
["Email Alert","●","●","●","●","●","●","●"]
["DI/DO"]
["Certification"]
["UL60950-1","●"]
["UL508",null,"●","●","●","●"]
["UL61010",null,null,null,null,null,"●","●"]
["UL-C1D2"]
["3C","●"]
["FCC","●","●","●","●","●","●","●"]
["CE","●","●","●","●","●","●","●"]
["Others",null,"EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2","EN 50121-4\nNEMA TS2"]

{"sheet":"DS - Train Switch","index":15,"n_rows":86,"n_cols":12,"rows_kept":86,"cut":false,"hidden":false,"merged":[[0,1,0,7],[0,10,0,11]]}
[null,"Managed M12 Switch",null,null,null,null,null,null,null,null,"Unmanaged M12 Switch"]
[null,"EKI-6558TI","EKI-6559TMI","EKI-9512","EKI-9512P","EKI-9516","EKI-9516P","EKI-7624E-PI",null,null,"EKI-6528TI","EKI-6528TPI"]
["Connectivity",null,null,null,null,null,null,null,null,"Connectivity"]
["10/100Base-TX, Fixed",8,8,null,null,null,null,null,null,"10/100Base-Tx, fixed","8 (2 Auto-Bypass)","4 (2 Auto-Bypass)"]
["10/100Base-TX PoE, fixed",null,null,null,null,null,null,24,null,"10/100Base-TX PoE, fixed",null,4]
["10/100/1000Based-T,Fixed",null,null,"12 (2-Pair Auto-Bypass)","4 (2-Pair Auto-Bypass)","16 (2-Pair Auto-Bypass)","4 (2-Pair Auto-Bypass)",null,null,"10/100/1000Based-Tx,fixed"]
["10/100/1000Based-T PoE,Fixed",null,null,null,8,null,12,null,null,"10/100/1000Based-T PoE,Fixed"]
["100FX Fiber, Fixed",null,2,null,null,null,null,null,null,"100FX Fiber, fixed"]
["100FX Fiber mode",null,"Multi-mode",null,null,null,null,null,null,"100FX Fiber mode"]
["100FX Fiber connector type",null,"LC",null,null,null,null,null,null,"100FX Fiber connector type"]
["Open SFP Slot (GbE)",null,null,null,null,null,null,null,null,"Auto MDI/MDI-X","●","●"]
["Open SFP Slot (Compatibility 100-FX)",null,null,null,null,null,null,null,null,"Auto Negotiation","●","●"]
["Performance",null,null,null,null,null,null,null,null,"Performance"]
["Switch Fabric Speed,Gbps","1.6Gbps","2Gbps","24Gbps","24Gbps","32Gbps","32Gbps","4.8Gbps",null,"Switch fabric speed,Gbps","1.6 Gbps","1.6 Gbps"]
["Forwarding Rate (Throughput, Mpps)","2.38096Mpps","2.9762Mpps","TBD","TBD","TBD","TBD","TBD",null,"Throughput, Mpps","2.38096Mpps","2.38096Mpps"]
["Packet buffer,Bytes","128KB","128KB","128KB","128KB","128KB","128KB","128KB",null,"Packet buffer","56KB","56KB"]
["MAC Address Table","8K","8K","16K","16K","16K","16K","8K",null,"MAC address table","2K","2K"]
["MTBF","388,201hrs","320,420 hrs","TBD","TBD","TBD","TBD","TBD",null,"MTBF","391,306hrs","348,384hrs"]
["Physical",null,null,null,null,null,null,null,null,"Physical"]
["Dimensions ( WxHxD )","193x176x62.5 mm","193x176x62.5 mm","254 x 174 x 64.5 mm","254 x 174 x 64.5 mm","254 x 174 x 64.5 mm","254 x 174 x 64.5 mm","380 x 157 x 90.65  mm",null,"Housing Dimensions ( WxHxD ) mm","92x180x42 mm","92x180x42 mm"]
["Mounting way","Wall mount","Wall mount","Wall mount","Wall mount","Wall mount","Wall mount","Wall mount",null,"Mounting way","Wall mount","Wall mount"]
["IP rating","IP67","IP67","IP67","IP67","IP67","IP67","IP40",null,"IP rating","IP30","IP30"]
["Power",null,null,null,null,null,null,null,null,"Power"]
["Power Input Voltage","12~48VDC","12~48VDC","24, 48, 72, 96, 110VDC (Wide Range)","24, 48VDC (Low Voltage)\n72, 110VDC (High Voltage)","24, 48, 72, 96, 110VDC (Wide Range)","24, 48VDC (Low Voltage)\n72, 110VDC (High Voltage)","48VDC",null,"Power Input voltage","12~48VDC","24~48VDC"]
["Dual Power Input","●","●","●","●","●","●","●",null,"Dual Power input","●","●"]
["Relay Output","●","●","●","●","●","●","●",null,"Relay output","●","●"]
["Power Consumption(Max, 48VDC)","3.84 Watts","8.1 Watts","26.4 Watts","116.4 Watts","26.4 Watts","116.4Watts","120 Watts",null,"Power Consumption","3.36W","72 Watts"]
["Input Reverse Protection","●","●","●","●","●","●","●",null,"Reverse protection","●","●"]
["L2 Feature",null,null,null,null,null,null,null,null,"Traffic Control"]
["IEEE 802.3x Flow Control ","●","●","●","●","●","●","●",null,"Broadcast Storm protection","●","●"]
["Static/802.3ad LACP (Link Aggregation Control Protocol)","●","●","●","●","●","●","●",null,"Jumbo frame size"]
["VLAN, Max. VLAN Supported",256,256,256,256,256,256,256,null,"IEEE 802.3x flow control","●","●"]
["Available VLAN ID Range","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094","1-4094",null,"Certification"]
["Port-Based VLAN ","●","●","●","●","●","●","●",null,"UL60950-1","●","●"]
["802.1Q VLAN Trunking ","●","●","●","●","●","●","●",null,"UL508"]
["802.1ad VLAN Stacking (QinQ) ",null,null,"●","●","●","●","●",null,"UL-C1D2"]
["GVRP (Generic VLAN Registration Protocol)","●","●","●","●","●","●","●",null,"3C","●","●"]
["GARP (Generic Attribute Registration Protocol)",null,null,null,null,null,null,null,null,"FCC","●","●"]
["Max Multicast Group Supported ","●","●","●","●","●","●","●",null,"CE","●","●"]
["IGMP Snooping (v1,v2)","●","●","●","●","●","●","●",null,"EN50155","●","●"]
["IGMP Querier","●","●","●","●","●","●","●"]
["IGMP Filtering ","●","●","●","●","●","●","●"]
["IPv6 ",null,null,"●","●","●","●"]
["Redudancy"]
["IEEE 802.1D (STP)","●","●","●","●","●","●","●"]
["IEEE 802.1w (RSTP)","●","●","●","●","●","●","●"]
["X-Ring (Advantech Propietary)","●","●","●","●","●","●","●"]
["Security"]
["802.1x (Port-Based)","●","●","●","●","●","●","●"]
["Port Security ","●","●","●","●","●","●","●"]
["Layer 2 MAC filtering ","●","●","●","●","●","●","●"]
["Quality of Service (QoS)"]
["802.1p Priority Queues per Port ",4,4,4,4,4,4,4]
["802.1p Queuing method ","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR","SPQ/WRR"]
["Class of Service (CoS)"]
["802.1p based COS","●","●","●","●","●","●","●"]
["IP TOS/Precedence based COS","●","●","●","●","●","●","●"]
["DSCP based COS","●","●","●","●","●","●","●"]
["TCP/UDP Port based COS"]
["Management"]
["CLI","●","●","●","●","●","●","●"]
["Web Based Management","●","●","●","●","●","●","●"]
["Telnet Management","●","●","●","●","●","●","●"]
["Console Management","●","●","●","●","●","●","●"]
["SNMP(v1,v2c)","●","●","●","●","●","●","●"]
["Backup/Restore(TFTP,HTTP)","●","●","●","●","●","●","●"]
["DNS","●","●","●","●","●","●","●"]
["DHCP Server","●","●","●","●","●","●","●"]
["DHCP Client","●","●","●","●","●","●","●"]
["Diagnostic"]
["Port Mirror","●","●","●","●","●","●","●"]
["SNMP(v1,v2c)","●","●","●","●","●","●","●"]
["RMON(1,2,3,9 Group)","●","●","●","●","●","●","●"]
["SNTP","●","●","●","●","●","●","●"]
["Event/Error Log(Local Flash)","●","●","●","●","●","●","●"]
["Real-Time Traffic Statistic","●","●","●","●","●","●","●"]
["SNMP Trap","●","●","●","●","●","●","●"]
["Email Alert","●","●","●","●","●","●","●"]
["Certification"]
["UL60950-1"]
["UL508","●","●","●","●","●","●"]
["UL-C1D2"]
["3C","●","●"]
["FCC","●","●","●","●","●","●","●"]
["CE","●","●","●","●","●","●","●"]
["EN50155","●","●","●","●","●","●","●"]

{"sheet":"DS - Device Server","index":16,"n_rows":63,"n_cols":28,"rows_kept":63,"cut":false,"hidden":false,"merged":[[51,1,51,9],[51,10,51,12],[51,13,51,19],[51,20,51,24],[51,25,51,27],[52,1,52,9],[52,10,52,12],[52,13,52,19],[52,20,52,23],[52,24,52,27],[0,1,0,12],[0,13,0,19],[0,20,0,24],[0,25,0,27],[49,1,49,9],[49,10,49,12],[49,13,49,19],[49,20,49,23],[49,24,49,27]]}
[null,"2015 - New Products",null,null,null,null,null,null,null,null,null,null,null,"EKI-1500 Series",null,null,null,null,null,null,"ADAM-4500 series",null,null,null,null,"EKI-1200 series"]
[null,"EKI-1521-BE","EKI-1521I-BE","EKI-1521CI-BE","EKI-1522-BE","EKI-1522I-BE","EKI-1522CI-BE","EKI-1524-BE","EKI-1524I-BE","EKI-1524CI-BE","EKI-1224-BE","EKI-1224I-BE","EKI-1224CI-BE","EKI-1521-AE","EKI-1522-AE","EKI-1524-AE","EKI-1528-BE","EKI-1526-BE","EKI-1528T-VDC-BE","EKI-1526T-VDC-BE","ADAM-4570-CE","ADAM-4570L-DE","ADAM-4571-CE","ADAM-4571L-DE","ADAM-4572-CE","EKI-1221-AE","EKI-1222-AE","EKI-1224-AE"]
["Device Server Classification"]
["Device Server","●","●","●","●","●","●","●","●","●",null,null,null,"●","●","●","●","●","●","●","●","●","●","●"]
["Modbus Gateway",null,null,null,null,null,null,null,null,null,"●","●","●",null,null,null,null,null,null,null,null,null,null,null,"●","●","●","●"]
["Programmable Device Server"]
["CPU","ARM11 300MHz","ARM11 300MHz","ARM11 300MHz","ARM11 300MHz","ARM11 300MHz","ARM11 300MHz","ARM11 300MHz","ARM11 300MHz","ARM11 300MHz","ARM11 300MHz","ARM11 300MHz","ARM11 300MHz","ARM7 80MHz","ARM7 80MHz","ARM7 80MHz","XScale 300MHz","XScale 300MHz","XScale 300MHz","XScale 300MHz","ARM7 80MHz","ARM7 80MHz","ARM7 80MHz","ARM7 80MHz","ARM7 80MHz","ARM7 80MHz","ARM7 80MHz","ARM7 80MHz"]
["Storage","32MB Flash","32MB Flash","32MB Flash","32MB Flash","32MB Flash","32MB Flash","32MB Flash","32MB Flash","32MB Flash","32MB Flash","32MB Flash","32MB Flash","8MB Flash","8MB Flash","8MB Flash","32MB Flash","32MB Flash","32MB Flash","32MB Flash","8MB Flash","8MB Flash","8MB Flash","8MB Flash","8MB Flash","8MB Flash","8MB Flash","8MB Flash"]
["Memory","128MB DDRII","128MB DDRII","128MB DDRII","128MB DDRII","128MB DDRII","128MB DDRII","128MB DDRII","128MB DDRII","128MB DDRII","128MB DDRII","128MB DDRII","128MB DDRII","16MB SDRAM","16MB SDRAM","16MB SDRAM","128MB DDR","128MB DDR","128MB DDR","128MB DDR","16MB SDRAM","16MB SDRAM","16MB SDRAM","16MB SDRAM","16MB SDRAM","16MB SDRAM","16MB SDRAM","16MB SDRAM"]
["Operation System","uClinux 2.6","uClinux 2.6","uClinux 2.6","uClinux 2.6","uClinux 2.6","uClinux 2.6","uClinux 2.6","uClinux 2.6","uClinux 2.6","uClinux 2.6","uClinux 2.6","uClinux 2.6","uClinux 2.4","uClinux 2.4","uClinux 2.4","uClinux 2.6","uClinux 2.6","uClinux 2.6","uClinux 2.6","uClinux 2.4","uClinux 2.4","uClinux 2.4","uClinux 2.4","uClinux 2.4","uClinux 2.4","uClinux 2.4","uClinux 2.4"]
["Ethernet Connectivity"]
["10/100Base-TX, Fixed",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,1,1,1,1,1,2,2,2]
["10/100/1000Based-T,Fixed"]
["Embedded Switch (Daisy-Chain)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
["Serial Connectivity"]
["RS-232 only",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,1]
["RS-422/485",null,null,1,null,null,2,null,null,4,null,null,4]
["RS-232/422/485",1,1,null,2,2,null,4,4,null,4,4,null,1,2,4,8,16,8,16,2,null,1,null,1,1,2,4]
["Serial connector type","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","RJ-45","RJ-45","RJ-45","RJ-45","10-pin RJ48","10-pin RJ48","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male"]
["Isolation",null,null,"●",null,null,"●",null,null,"●",null,null,"●"]
["Performance"]
["RTC","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●",null,null,null,null,null,"●","●","●"]
["HW Watch Dog Supported","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Physical"]
["Dimensions ( WxHxD )","37x140x95 mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","55x152x105 mm","55x152x105 mm","55x152x105 mm","55x152x105 mm","55x152x105 mm","55x152x105 mm","37x140x95 mm","37x140x95 mm","55x152x105 mm","40x440x220 mm","40x440x220 mm","40x440x220 mm","40x440x220 mm","130x70x30 mm","130x70x30 mm","130x70x30 mm","130x70x30 mm","130x70x30 mm","37x140x95 mm","37x140x95 mm","55x152x105 mm"]
["Weight,fully loaded, kg","0.592kg","0.592kg","0.592kg","0.6kg","0.6kg","0.6kg","0.668kg","0.668kg","0.668kg","0.668kg","0.668kg","0.668kg","0.592kg","0.6kg","0.668kg","2.53kg","2.58kg","2.53kg","2.58kg","0.16kg","0.16kg","0.135kg","0.135kg","0.135kg","0.592kg","0.6kg","0.668kg"]
["Enclusure & Mount kit"]
["Enclusure","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","IP30","SECC chassis","SECC chassis","SECC chassis","SECC chassis","ABS+PC","ABS+PC","ABS+PC","ABS+PC","ABS+PC","IP30","IP30","IP30"]
["DIN-rail","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●",null,null,null,null,"●","●","●","●","●","●","●","●"]
["Panel","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●",null,null,null,null,null,null,null,null,null,"●","●","●"]
["Wall","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●",null,null,null,null,"●","●","●","●","●","●","●","●"]
["rack size",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1U","1U","1U","1U"]
["Stack",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●","●","●"]
["Power"]
["Power Input Voltage","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","110~240VAC/VDC","110~240VAC/VDC","48VDC","48VDC","10~30VDC","10~30VDC","10~30VDC","10~30VDC","10~30VDC","12~48VDC","12~48VDC","12~48VDC"]
["Power connector","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block",null,null,"Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block"]
["Power Consumption","5.2W","5.2W","5.2W","5.2W","5.2W","5.2W","6.3W","6.3W","6.3W","6.3W","6.3W","6.3W","2W","2.5W","4W","8W","10W","8W","10W","1.5W","1.5W","1.5W","1.5W","1.5W","2W","2.5W","4W"]
["Environment"]
["Wide Temp.",null,"●","●",null,"●","●",null,"●","●",null,"●","●"]
["Operating Temp.","-10 ~ 60","-40 ~ 70","-40 ~ 70","-10 ~ 60","-40 ~ 70","-40 ~ 70","-10 ~ 60","-40 ~ 70","-40 ~ 70","-10 ~ 60","-40 ~ 70","-40 ~ 70","-10 ~ 60","-10 ~ 60","-10 ~ 60","-10 ~ 60","-10 ~ 60","-10 ~ 60","-10 ~ 60","-10 ~ 60","-10 ~ 60","-10 ~ 60","-10 ~ 60","0 ~ 60","-10 ~ 60","-10 ~ 60","-10 ~ 60"]
["Operating Humidity"]
["Operating Humility","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%"]
["Input Reverse Protection","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●",null,"●"]
["Configuration"]
["Windows Utility","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Web Interface","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Telnet","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["Standalone Console Port",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●","●"]
["Software"]
["Netwrok Protocol","ICMP, IPv4, IPv6, TCP, UDP, BOOTP, DHCP, Auto IP, Telnet, SNMP, HTTP, DNS, SMTP, ARP, NTP,  HTTPS, SSL, SSH",null,null,null,null,null,null,null,null,"Modbus TCP, Modbus RTU/ASCII",null,null,"ICMP, IP, TCP, UDP, BOOTP, DHCP, Auto IP, Telnet, SNMP, HTTP, DNS, SMTP, ARP, NTP,  HTTPS, SSL, SSH",null,null,null,null,null,null,"ICMP, IP, TCP, UDP, BOOTP, DHCP, Auto IP, Telnet, SNMP, HTTP, DNS, SMTP, ARP",null,null,null,"Modbus TCP, Modbus RTU/ASCII"]
["IPv6/IPv4 Dual Stack","●","●","●","●","●","●","●","●","●"]
["Management","SNMP MIB-II",null,null,null,null,null,null,null,null,"SNMP MIB-II",null,null,"SNMP MIB-II",null,null,null,null,null,null,null,null,null,null,null,"SNMP MIB-II"]
["Standard operation mode","VCOM, TCP/UDP server, TCP/UDP client, Control Mode, RFC2217",null,null,null,null,null,null,null,null,"Modbus RTU Master/Slave, Modbus ASCII Master/Slave",null,null,"VCOM, TCP/UDP server, TCP/UDP client, Control Mode, RFC2217",null,null,null,null,null,null,"VCOM, TCP/UDP server, TCP/UDP client, Pair connection",null,null,null,"Modbus RTU Master/Slave, Modbus ASCII Master/Slave"]
["Port Buffering","●","●","●","●","●","●","●","●","●"]
["Secure operation mode"]
["Certification"]
["CE(EN55022 class A, EN55024)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["FCC (part 15 subpart B class A)","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●","●"]
["UL60950-1",null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●",null,null,null,null,null,null,null,null,null,"●","●","●"]
["EN60950-1",null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●",null,null,null,null,null,null,null,null,null,"●","●","●"]
["Hazardous Location (Class I, Division 2)",null,null,null,null,null,null,null,null,null,null,null,null,"●","●","●",null,null,null,null,null,null,null,null,null,"●","●","●"]
["MTBF",null,null,null,null,null,null,null,null,null,null,null,null,"215,266 hrs","337,238 hrs","337,238 hrs","249,812hrs","227,175hrs","249,812 hrs","227,175 hrs","264,964hrs","218,490hrs","262,230hrs",null,"3,094,713 hrs","109,064hrs","388,201hrs","337,238 hrs"]
["EMC Level",4,4,4,4,4,4,4,4,4,4,4,4,2,2,2,2,2,2,2,3,3,3,3,3,2,2,2]

{"sheet":"DS - Media Converter","index":17,"n_rows":38,"n_cols":11,"rows_kept":38,"cut":false,"hidden":false,"merged":[[0,1,0,3],[0,4,0,5],[0,6,0,10]]}
[null,"2015 - New Products",null,null,null,null,"EKI-2000 Series"]
[null,"EKI-3741F/FI","EKI-3541M-ST","EKI-3541S-ST","EKI-3541M","EKI-3541S","EKI-2541M/MI","EKI-2541S/SI","EKI-2741F","EKI-2741LX/LXI","EKI-2741SX"]
["Connectivity"]
["10/100Base-Tx, fixed",null,1,1,1,1,1,1]
["10/100/1000Based-Tx,fixed",1,null,null,null,null,null,null,1,1,1]
["100FX Fiber, fixed",null,1,1,1,1,1,1]
["1000Base Fiber, fixed",1,null,null,null,null,null,null,null,1,1]
["Fiber mode",null,"Multi-mode","Single-mode","Multi-mode","Single-mode","Multi-mode","Single-mode",null,"Single-mode","Multi-mode"]
["Fiber connector type",null,"ST","ST","SC","SC","SC","SC",null,"SC","SC"]
["Open SFP slot (GbE)",1,null,null,null,null,null,null,1]
["Open SFP Slot (Compatibility 100-FX)"]
["Performance"]
["Auto MDI/MDI-X","●","●","●","●","●","●","●","●","●","●"]
["Auto Negotiation","●","●","●","●","●","●","●","●","●","●"]
["Store-and-Forward Switching ","●","●","●","●","●","●","●","●","●","●"]
["Link Lose Forwarding (LLF) by DIP switch",null,"●","●","●","●","●","●","●","●","●"]
["Link Fault Pass-Through (LFP) by DIP switch","●","●","●","●","●","●","●","●","●","●"]
["MTBF","TBD","597,488Hrs","597,488Hrs","597,488Hrs","597,488Hrs"]
["Traffic Control"]
["Jumbo frame size","9Kbytes","1600 byte","1600 byte","1600 byte","1600 byte",null,null,"9Kbytes"]
["IEEE 802.3x flow control","Yes","Yes","Yes","Yes","Yes","●","●","●","●","●"]
["Physical"]
["Housing Dimensions \n(  WxHxD ) mm","28.5 x 120 x 85.3 mm ","28.5 x 120 x 85.3 mm ","28.5 x 120 x 85.3 mm ","28.5 x 120 x 85.3 mm ","28.5 x 120 x 85.3 mm ","37x140x95 mm","37x140x95 mm","37x140x95 mm","37x140x95 mm","48.6x140x95 mm"]
["Mounting way","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount","DIN-Rail/Wall mount"]
["IP rating","IP40","IP40","IP40","IP40","IP40","IP30","IP30","IP30","IP30","IP30"]
["Power"]
["Power Input voltage","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","12~48VDC","24~48VDC"]
["Dual Power input","●","●","●","●","●","●","●","●","●","●"]
["Relay output","●","●","●","●","●","●","●","●","●","●"]
["Power Consumption","TBD","2.4W","2.4W","2.4W","2.4W","2.7W","5W","5.28W","5.30W","5.18W"]
["Reverse protection","●","●","●","●","●","●","●","●","●","●"]
["Certification"]
["UL60950-1","●","●","●","●","●","●","●","●","●","●"]
["UL508"]
["UL-C1D2",null,null,null,null,null,"●","●","●","●","●"]
["3C",null,null,null,null,null,"●","●","●","●","●"]
["FCC","●","●","●","●","●","●","●","●","●","●"]
["CE","●","●","●","●","●","●","●","●","●","●"]

{"sheet":"DS - Wireless Connectivity","index":18,"n_rows":63,"n_cols":12,"rows_kept":63,"cut":false,"hidden":false,"merged":[[0,4,0,7],[0,8,0,11],[37,1,37,2],[37,10,37,11],[0,1,0,2]]}
[null,"WiFi AP/Client",null,"WiFi Client","EKI-1360 series",null,null,null,"EKI-1300 celleular series"]
[null,"EKI-6332GN-AE","EKI-6331AN-BE","EKI-6232GN-AE","EKI-1361","EKI-1361-MB","EKI-1362","EKI-1362-MB","EKI-1321","EKI-1322","EKI-1331","EKI-1334"]
["Connectivity"]
["10/100Base-TX, Fixed",1,1,1,1,1,1,1,1,1,1,5]
["10/100/1000Based-T,Fixed","-","-","-","-","-","-","-","-","-","-","-"]
["RS-232 only","-","-","-","-","-","-","-","-","-","-",1]
["RS-232/422/485","-","-","-",1,1,2,2,1,2,1,"-"]
["Serial connector type","-","-","-","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","DB9 Male","Terminal block","DB9 Male"]
["Operating Mode"]
["Mobility/Roaming","●","●","●","●","●","●","●","●","●","●","●"]
["Multi-Hopping","●","●","●","-","-","-","-","-","-","-","-"]
["AP/CPE","●","●","-","-","-","-","-","-","-","-","-"]
["Performance"]
["HW Watch Dog Supported","●","●","-","●","●","●","●","●","●","●","●"]
["MTBF",null,null,null,null,null,null,null,"250,472hrs","249,547hrs","410,340hrs","410,340hrs"]
["Physical"]
["Dimensions ( WxHxD )","111x256x48 mm","111x256x48 mm","85x120x25mm","27 x 120 x 85 mm","27 x 120 x 85 mm","27 x 120 x 85 mm","27 x 120 x 85 mm","27x120x85 mm","27x120x85 mm"," 45 x 90 x 80mm","45 x 133 x 113 mm"]
["Weight,fully loaded, kg","0.5kg","0.5Kg","0.2kg","0.495 Kg","0.495 Kg","0.503 Kg","0.503 Kg","0.49kg","0.5kg","0.34kg","0.34kg"]
["Enclusure & Mount kit"]
["Enclusure","IP55","IP55","IP30","IP40","IP40","IP40","IP40","IP30","IP30","IP30","IP30"]
["DIN-rail","-","-","-","●","●","●","●","●","●","●","●"]
["Wall","●","●","●","●","●","●","●","●","●","●","●"]
["VESA Mount","-","-","-","-","-","-","-","-","-","-","-"]
["Pole Mount","●","●","-","-","-","-","-","-","-","-","-"]
["Power"]
["Power Input (VDC)","24VDC","24VDC","12~48VDC ","2*(12~48V)","2*(12~48V)","2*(12~48V)","2*(12~48V)","2*(12~48V)","2*(12~48V)","(12~24V)","(9~26V)"]
["Power input (PoE)","-","-","-","-","-","-","-","-","-","-","-"]
["Power connector","RJ45","RJ45","RJ45","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block","Terminal block"]
["Power Consumption (12/24/48VDC) Watts",null,null,null,"8W","8W","9W","9W"]
["Environment"]
["Operating Temp.","-20 ~ 70","-20 ~ 70","-20 ~ 75","-30 ~ 65","-30 ~ 65","-30 ~ 65","-30 ~ 65","-35 ~ 65","-35 ~ 65","-20 ~ 70","-20 ~ 70"]
["Operating Humidity"]
["Operating Humility","10 ~ 95%","10 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%","5 ~ 95%"]
["Input Reverse Protection","-","-","-","●","●","●","●","●","●","●","●"]
["Software"]
["Firewall","MAC/IP/Port filter","MAC/IP/Port filter","MAC/IP/Port filter","-","-","-","-","NAT, port forwarding","NAT, port forwarding","NAT","NAT"]
["Netwrok Protocol",null,null,null,null,"Modbus TCP, Modbus RTU/ASCII",null,"Modbus TCP, Modbus RTU/ASCII"]
["configuration option","Web-base",null,"Web-base/Advantech EKI Devices Utility","Web-base, windows utility","Web-base, windows utility","Web-base, windows utility","Web-base, windows utility","Web-base, windows utility",null,"Telnet console, Web-base"]
["Authentication","Username/Password","Username/Password","Username/Password","Username/Password","Username/Password","Username/Password","Username/Password","Username/Password","Username/Password","Username/Password","Username/Password"]
["Standard operation mode","AP/CPE","AP/CPE","CPE","VCOM, USDG mode(TCP/UDP server, TCP/UDP client), Pair connection/Access Point Mode"," Pair connection/Access Point Mode/\nModbus RTU Master/Slave, Modbus ASCII Master/Slave","VCOM, USDG mode(TCP/UDP server, TCP/UDP client), Pair connection/Access Point Mode","Pair connection/Access Point Mode/\nModbus RTU Master/Slave, Modbus ASCII Master/Slave","VCOM, USDG mode(TCP/UDP server, TCP/UDP client), Pair connection, RFC2217, SMS tunnel, IP Gateway w/ VPN","VCOM, USDG mode(TCP/UDP server, TCP/UDP client), Pair connection, RFC2217, SMS tunnel, IP Gateway w/ VPN","Modbus RTU & TCP, USDG mode(TCP/UDP server mode, TCP/UDP client mode), IP \nGateway w/ VPN","Modbus RTU & TCP, USDG mode(TCP/UDP server mode, TCP/UDP client mode), IP \nRouter w/ VPN"]
["WLAN"]
["IEEE Standard","802.11b/g/n","802.11a/n","802.11b/g/n","802.11b/g/n","802.11b/g/n","802.11b/g/n","802.11b/g/n","-","-","-","-"]
["Radio Number",1,1,1,1,1,1,1,1,1,1,1]
["Security","WEP, 802.1X, WPA, WPA2, WPA&WPA2,WPA-PSK, WPA2-\nPSK, WPA-PSK&WPA2-PSK","WEP, 802.1X, WPA, WPA2, WPA&WPA2,WPA-PSK, WPA2-\nPSK, WPA-PSK&WPA2-PSK","WEP, WPA/WPA2-personal, WPA/WPA2-enterprise","WEP, WPA/WPA2-Personal, WPA/WPA2-Enterprise","WEP, WPA/WPA2-Personal, WPA/WPA2-Enterprise","WEP, WPA/WPA2-Personal, WPA/WPA2-Enterprise","WEP, WPA/WPA2-Personal, WPA/WPA2-Enterprise"]
["RF"]
["MIMO","2T2R","2T2R","2T2R","2T2R","2T2R","2T2R","2T2R","-","-","-","-"]
["Maximum Transmit Output Power ","27dBm (11b)","23dBm (11a)","20dBm (11b)","19dBm (11n)","19dBm (11n)","19dBm (11n)","19dBm (11n)","Class 4 (2 W) for EGSM850\nClass 4 (2 W) for EGSM900\n Class 1 (1 W) for GSM1800\nClass 1 (1 W) for GSM1900","Class 4 (2 W) for EGSM850\nClass 4 (2 W) for EGSM900\n Class 1 (1 W) for GSM1800\nClass 1 (1 W) for GSM1900","HSDPA Cat. 10 / HSUPA Cat.6 data rates \nDGE class 12 data rates: \nGPRS class 12 data rates","HSDPA Cat. 10 / HSUPA Cat.6 data rates \nDGE class 12 data rates: \nGPRS class 12 data rates"]
["Rcecive Sensitivity","-91dBm (11b 1Mbps)","-89dBm (11a 6Mbps)","-86dBm (11b 1Mbps)","-93dBm (11g Rx0+Rx1)","-93dBm (11g Rx0+Rx1)","-93dBm (11g Rx0+Rx1)","-93dBm (11g Rx0+Rx1)","-102dBm","-102dBm","-102dBm","-102dBm"]
["Antenna Connector","R-SMA","R-SMA","R-SMA","R-SMA","R-SMA","R-SMA","R-SMA","SMA","SMA","SMA","SMA"]
["Cellular"]
["Standard","-","-","-","-","-","-","-","GPRS (class 10)","GPRS (class 10)","HSUPA Cat.6","HSUPA Cat.6"]
["Five-band option in UMTS","-","-","-","-","-","-","-",null,null,"●","●"]
["Quad-band optin in EDGE/GSM","-","-","-","-","-","-","-","●","●","●","●"]
["Certification (GCF, PTCRB)","-","-","-","-","-","-","-","●","●","●","●"]
["Certification"]
["UL60950-1",null,null,null,"●","●","●","●","-","-","-","-"]
["EN60950-1","●","●","-","●","●","●","●","-","-","-","-"]
["CE(EN55022 class A, EN55024)","●","●","-","●","●","●","●","●","●","●","●"]
["FCC (part 15 subpart B class A)","●","●","-","●","●","●","●","●","●","-","-"]
["Hazardous Location (Class I, Division 2)","-","-","-","-","-","-","-","-","-","-","-"]
["Radio (EN 301 489-1/-4, EN 301 511)","●","●","-",null,null,null,null,"●","●","●","●"]
["Radio (FCC part 22H, part 24H)",null,null,null,null,null,null,null,"●","●","●","●"]
["EN 50155","-","-","-",null,null,null,null,"-","-","-","-"]

{"sheet":"DS - NMS","index":19,"n_rows":43,"n_cols":2,"rows_kept":43,"cut":false,"hidden":false,"merged":[]}
["Model","WebAccess/NMS"]
["Features"]
["Interface","Web"]
["Auto Scan","●"]
["Auto Topology","●"]
["Trend-Chart Monitoring","●"]
["Performance Monitoring","●"]
["Event/Log Management","●"]
["Batch Firmware Upgrade","●"]
["Schedule Firmware Upgrade","●"]
["Accounting","●"]
["Authorization","●"]
["Topology View Background"]
["Google Map","●"]
["Open Street Map","●"]
["Static Bitmap/Image","●"]
["Capability"]
["Maximum Support Nodes",4000]
["Free Trail Nodes",200]
["Acceptable Traps/syslog per Second",500]
["License","USB Key Pro"]
["Networl Protocol Support"]
["Wireless","●"]
["Cellular","●"]
["X-Ring","●"]
["LLDP","●"]
["SNMP","●"]
["STP/RSTP","●"]
["Device Connection Indication"]
["Link Status","●"]
["Port Trunk","●"]
["Ring Backup Path","●"]
["Wireless Connection","●"]
["Cellular Connection","●"]
["Notification"]
["SMS","●"]
["eMail","●"]
["Trap","●"]
["Event Log","●"]
["OS Support"]
["Windows","●"]
["Database Support"]
["Microsoft SQL Server","●"]